{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXF-B"]
[]
[]
[]
[]
["","","","","","2AMXF40B2V1B","2AMXF50B2V1B"]
["Rozměry","Jednotka","","Výška","mm","550","550"]
["","","","Šířka","mm","765","765"]
["","","","Hloubka","mm","285","285"]
["Hmotnost","Jednotka","","","kg","36","41"]
["Motor ventilátoru","Otáčky","Chlazení","Velmi nízké","ot./min","500","500"]
["","","Vytápění","Velmi nízké","ot./min","320","500"]
["Kompresor","Typ","","","","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","46","48"]
["","Vytápění","","Vysoké","dBA","48","50"]
["Chladivo","Typ","","","","R-32","R-32"]
["","Náplň","","","kg","0.84","1.09"]
["","Náplň","","","tCO2Eq","0.57","0.74"]
["","Vliv na globální oteplování (GWP)","","","","675","675"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","20 (1)","20 (1)"]
["","Doplňková náplň chladiva","","","kg/m","0,02 (pro délku potrubí přesahující 20m)","0,02 (pro délku potrubí přesahující 20m)"]
["","Rozdíl hladin","IU - OU","Max.","m","15.0","15.0"]
["","","IU - IU","Max.","m","7.5","7.5"]
["","Celková délka potrubí","Systém","Skutečná","m","30.0","30.0"]
["Standardní příslušenství","Příručka pro instalaci","","","","1","1"]
["","Uzávěr vypouštění","","","","1","1"]
["","Sáček se šrouby","","","","1","1"]
["Energetickou účinná řada","","","","","A+++ ~ D","A+++ ~ D"]
["Napájení","Fáze","","","","1~","1~"]
["","Frekvence","","","Hz","50","50"]
["","Napětí","","","V","220-230-240","220-230-240"]
["Poznámky","","","","","(1) - Jedna místnost","(1) - Jedna místnost"]
["","","","","","(2) - Viz samostatný výkres s provozním rozsahem","(2) - Viz samostatný výkres s provozním rozsahem"]
["","","","","","(3) - Údaje o elektrickém systému najdete v samostatném výkresu","(3) - Údaje o elektrickém systému najdete v samostatném výkresu"]
["","","","","","(4) - Obsahuje fluorované skleníkové plyny","(4) - Obsahuje fluorované skleníkové plyny"]
["Standardní příslušenství","Sestava reduktoru","","","","","1"]