{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-A8"]
[]
[]
[]
[]
["","","","","","2MXM50A2V1B8","2MXM68A2V1B8"]
["Rozměry","Jednotka","","Výška","mm","552","734"]
["","","","Šířka","mm","852","974"]
["","","","Hloubka","mm","350","408"]
["Hmotnost","Jednotka","","","kg","41","60"]
["Kompresor","Typ","","","","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","50","50"]
["Hladina akustického tlaku","Chlazení","","Jm.","dBA","48","48"]
["","Vytápění","","Jm.","dBA","50","48"]
["Chladivo","Typ","","","","R-32","R-32"]
["","Náplň","","","kg","1.15","2.00"]
["","Náplň","","","tCO2Eq","0.78","1.35"]
["","Vliv na globální oteplování (GWP)","","","","675","675"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","20 (1)","25 (1)"]
["","Doplňková náplň chladiva","","","kg/m","0,02 (pro délku potrubí přesahující 20m)","0,02 (pro délku potrubí přesahující 30m)"]
["","Rozdíl hladin","IU - OU","Max.","m","15","15"]
["","","IU - IU","Max.","m","7.5","7.5"]
["","Celková délka potrubí","Systém","Skutečná","m","30","50"]
["Standardní příslušenství","Installation manual","","","","1","1"]
["","Drain cap","","","","","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Napájení","Fáze","","","","1~","1~"]
["","Frekvence","","","Hz","50","50"]
["","Napětí","","","V","220-240","220-240"]
["Poznámky","","","","","(1) - Jedna místnost","(1) - Jedna místnost"]
["","","","","","(2) - Pro kombinaci s CVXM-A, FVXM-A – maximální délka potrubí 30m.","(2) - Pro kombinaci s CVXM-A, FVXM-A – maximální délka potrubí 30m."]
["","","","","","(3) - Viz samostatný výkres s provozním rozsahem","(3) - Viz samostatný výkres s provozním rozsahem"]
["","","","","","(4) - Údaje o elektrickém systému najdete v samostatném výkresu","(4) - Údaje o elektrickém systému najdete v samostatném výkresu"]
["","","","","","(5) - Obsahuje fluorované skleníkové plyny","(5) - Obsahuje fluorované skleníkové plyny"]