{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":9,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-M"]
[]
[]
[]
[]
["","","","","","2MXM40M2V1B","2MXM40M4V1B","2MXM40M3V1B","2MXM50M2V1B"]
["Ventilátor","Průtok vzduchu","Chlazení","Velmi nízké","m³/min","30","","","34"]
["","","Vytápění","Velmi nízké","m³/min","32","","","34"]
["","","","Velmi nízké","cfm","1059","","","1200"]
["","","Vytápění","Velmi nízké","cfm","1130","","","1200"]
["Rozměry","Jednotka","","Výška","mm","550","550","550","550"]
["","","","Šířka","mm","765","765","765","765"]
["","","","Hloubka","mm","285","285","285","285"]
["Hmotnost","Jednotka","","","kg","36","36","36","41"]
["Motor ventilátoru","Otáčky","Chlazení","Velmi nízké","ot./min","760","500","500","890"]
["","","Vytápění","Velmi nízké","ot./min","820","320","320","890"]
["Kompresor","Typ","","","","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CDB","-10","-10","-10 (2)","-10"]
["","","","Max.","°CDB","46","46","46 (2)","46"]
["","Vytápění","Okolí","Min.","° CWB","-15","-15","-15","-15"]
["","","","Max.","° CWB","18","18","18","18"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","","46","46"]
["","","","Jm.","dBA","48","","","46"]
["","Vytápění","","Vysoké","dBA","","48","48"]
["","","","Jm.","dBA","50","","","48"]
["Chladivo","Typ","","","","R-32","R-32","R-32","R-32"]
["","Náplň","","","kg","0.88","0.88","0.88","1.15"]
["","Náplň","","","tCO2Eq","0.6","0.60","0.59","0.8"]
["","Vliv na globální oteplování (GWP)","","","","675","675","675","675"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","20","20","20 (1)","20"]
["","Doplňková náplň chladiva","","","kg/m","0,02 (pro délku potrubí přesahující 20m)","0,02 (pro délku potrubí přesahující 20m)","0,02 (pro délku potrubí přesahující 20m)","0,02 (pro délku potrubí přesahující 20m)"]
["","Rozdíl hladin","IU - OU","Max.","m","15","15.0","15.0","15"]
["","","IU - IU","Max.","m","7.5","7.5","7.5","7.5"]
["","Celková délka potrubí","Systém","Skutečná","m","30","30","30","30"]
["Standardní příslušenství","Installation manual","","","","Installation manual","1","1","1"]
["","Drain plug","","","","Drain plug","1","1","1"]
["","Screw bag","","","","Screw bag","1","1","1"]
["Napájení","Fáze","","","","1~","1~","1~","1~"]
["","Frekvence","","","Hz","50","50","50","50"]
["","Napětí","","","V","220-240","220-230-240","220-230-240","220-240"]
["Poznámky","","","","","","(1) - Jedna místnost"]
["","","","","","","","(1) - Jedna místnost"]
["","","","","","","","(2) - Viz samostatný výkres s provozním rozsahem"]
["Standardní příslušenství","Reducer assembly","","","","","","","1"]