{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXS-H"]
[]
[]
[]
[]
["","","","","","2MXS40H3V1B2","2MXS40H3V1B","2MXS40H2V1B","2MXS50H3V1B2","2MXS50H3V1B","2MXS50H2V1B"]
["Hladina akustického tlaku","Vytápění","","Jm.","dBA","48","48","","50","50"]
["","Chlazení","","Jm.","dBA","47","47","","48","48"]
["Standardní příslušenství","Příručka pro instalaci","","","","1","1","","1","1"]
["","Sáček se šrouby","","","","1","1","","1","1"]
["","Uzávěr vypouštění","","","","1","1","","1","1"]
["Chladivo","Charge","","","TCO2Eq","2.5","2.5","","3.3","3.3"]
["","Vliv na globální oteplování (GWP)","","","","2,087.5","2,087.5","","2,087.5","2,087.5"]
["","Náplň","","","kg","1.20","1.20","","1.60","1.60"]
["","Typ","","","","R-410A","R-410A","","R-410A","R-410A"]
["Připojovací rozměry","Rozdíl hladin","IU - IU","Max.","m","7.5","7.5","","7.5","7.5"]
["","","IU - OU","Max.","m","15","15","","15","15"]
["","Doplňková náplň chladiva","","","kg/m","0,02 (pro délku potrubí přesahující 20m)","0,02 (pro délku potrubí přesahující 20m)","","0,02 (pro délku potrubí přesahující 20m)","0,02 (pro délku potrubí přesahující 20m)"]
["","Celková délka potrubí","Systém","Skutečná","m","30","30","","30","30"]
["Kompresor","Typ","","","","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor","","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor"]
["Rozměry","Jednotka","","Šířka","mm","765","765","","765","765"]
["","","","Hloubka","mm","285","285","","285","285"]
["","","","Výška","mm","550","550","","550","550"]
["Hmotnost","Jednotka","","","kg","38","38","","42","42"]
["Power supply","Phase","","","","1~","1~","","1~","1~"]
["","Frekvence","","","Hz","50","50","","50","50"]
["","Napětí","","","V","220-240","220-240","","220-240","220-240"]
["Poznámky","","","","","(1) - Obsahuje fluorované skleníkové plyny","(1) - Obsahuje fluorované skleníkové plyny","","(1) - Obsahuje fluorované skleníkové plyny","(1) - Obsahuje fluorované skleníkové plyny"]
["Rozměry","Jednotka","","Výška","mm","","","550","","","550"]
["","","","Šířka","mm","","","765","","","765"]
["","","","Hloubka","mm","","","285","","","285"]
["Hmotnost","Jednotka","","","kg","","","38","","","42"]
["Kompresor","Typ","","","","","","Hermeticky utěsněný rotační kompresor","","","Hermeticky utěsněný rotační kompresor"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CDB","","","10","","","10"]
["","","","Max.","°CDB","","","46","","","46"]
["","Vytápění","Okolí","Min.","° CWB","","","-15","","","-15"]
["","","","Max.","° CWB","","","15.5","","","15.5"]
["Hladina akustického tlaku","Chlazení","","Jm.","dBA","","","47","","","48"]
["","Vytápění","","Jm.","dBA","","","48","","","50"]
["Chladivo","Typ","","","","","","R-410A","","","R-410A"]
["","Náplň","","","kg","","","1.20","","","1.60"]
["","Náplň","","","tCO2Eq","","","2.5","","","3.3"]
["","Vliv na globální oteplování (GWP)","","","","","","2087.5","","","2087.5"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","","","20","","","20"]
["","Doplňková náplň chladiva","","","kg/m","","","0,02 (pro délku potrubí přesahující 20m)","","","0,02 (pro délku potrubí přesahující 20m)"]
["","Rozdíl hladin","IU - OU","Max.","m","","","15","","","15"]
["","","IU - IU","Max.","m","","","7.5","","","7.5"]
["","Celková délka potrubí","Systém","Skutečná","m","","","30","","","30"]
["Standardní příslušenství","Installation manual","","","","","","1","","","1"]
["","Drain plug","","","","","","1","","","1"]
["","Screw bag","","","","","","1","","","1"]
["Napájení","Fáze","","","","","","1~","","","1~"]
["","Frekvence","","","Hz","","","50","","","50"]
["","Napětí","","","V","","","220-240","","","220-240"]
["Standardní příslušenství","Sestava reduktoru","","","","","","","1","1"]
["","Reducer assembly","","","","","","","","","1"]