{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":68,"n_cols":7,"rows_kept":68,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3AMXM-M"]
[]
[]
[]
[]
["","","","","","3AMXM52M3V1B","3AMXM52M2V1B"]
["Hladina akustického tlaku","Vytápění","","Jm.","dBA","47"]
["","Chlazení","","Jm.","dBA","46"]
["Standardní příslušenství","Příručka pro instalaci","","","","1"]
["","Sáček se šrouby","","","","1"]
["","Uzávěr vypouštění","","","","1"]
["","Krytka vypouštění (1)","","","","6"]
["","Krytka vypouštění (2)","","","","3"]
["","Odlepovací štítek pro F-plyny","","","","1"]
["","Štítek dalších chladiv","","","","1"]
["Chladivo","Charge","","","TCO2Eq","1.2"]
["","Vliv na globální oteplování (GWP)","","","","675"]
["","Charge","","","kg","1.8"]
["","Typ","","","","R-32"]
["Motor ventilátoru","Otáčky","Chlazení","Velmi nízké","ot./min","420"]
["","","Vytápění","Velmi nízké","ot./min","420"]
["Piping connections","Rozdíl hladin","IU - IU","Max.","m","7.5"]
["","","IU - OU","Max.","m","15"]
["","Doplňková náplň chladiva","","","kg/m","0,02 (pro délku potrubí přesahující 30m)"]
["","Celková délka potrubí","Systém","Skutečná","m","50"]
["Kompresor","Typ","","","","Hermeticky utěsněný rotační kompresor"]
["Rozměry","Jednotka","","Šířka","mm","868"]
["","","","Hloubka","mm","320"]
["","","","Výška","mm","734"]
["Hmotnost","Jednotka","","","kg","57"]
["Power supply","Phase","","","","1~"]
["","Frekvence","","","Hz","50"]
["","Napětí","","","V","220-240"]
["Poznámky","","","","","(1) - Obsahuje fluorované skleníkové plyny"]
["","","","","","(2) - Viz samostatný výkres s provozním rozsahem"]
["","","","","","(3) - Údaje o elektrickém systému najdete v samostatném výkresu"]
["Ventilátor","Průtok vzduchu","Chlazení","Velmi nízké","m³/min","","24"]
["","","Vytápění","Velmi nízké","m³/min","","24"]
["","","","Velmi nízké","cfm","","847"]
["","","Vytápění","Velmi nízké","cfm","","847"]
["Rozměry","Jednotka","","Výška","mm","","734"]
["","","","Šířka","mm","","868"]
["","","","Hloubka","mm","","320"]
["Hmotnost","Jednotka","","","kg","","57"]
["Motor ventilátoru","Otáčky","Chlazení","Velmi nízké","ot./min","","420"]
["","","Vytápění","Velmi nízké","ot./min","","420"]
["Kompresor","Typ","","","","","Hermeticky utěsněný rotační kompresor"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CDB","","-10"]
["","","","Max.","°CDB","","46"]
["","Vytápění","Okolí","Min.","° CWB","","-15"]
["","","","Max.","° CWB","","18"]
["Hladina akustického tlaku","Chlazení","","Jm.","dBA","","46"]
["","Vytápění","","Jm.","dBA","","47"]
["Chladivo","Typ","","","","","R-32"]
["","Náplň","","","kg","","1.80"]
["","Náplň","","","tCO2Eq","","1.2"]
["","Vliv na globální oteplování (GWP)","","","","","675"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","","25"]
["","Doplňková náplň chladiva","","","kg/m","","0,02 (pro délku potrubí přesahující 30m)"]
["","Rozdíl hladin","IU - OU","Max.","m","","15"]
["","","IU - IU","Max.","m","","7.5"]
["","Celková délka potrubí","Systém","Skutečná","m","","50"]
["Standardní příslušenství","Installation manual","","","","","1"]
["","Drain plug","","","","","1"]
["","Screw bag","","","","","1"]
["Napájení","Fáze","","","","","1~"]
["","Frekvence","","","Hz","","50"]
["","Napětí","","","V","","220-240"]