{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-N7"]
[]
[]
[]
[]
["","","","","","3MXM40N2V1B7","3MXM52N2V1B7","3MXM68N2V1B7"]
["Ventilátor","Průtok vzduchu","Chlazení","Velmi nízké","m³/min","","","24.1"]
["","","Vytápění","Velmi nízké","m³/min","","","24.1"]
["","","","Velmi nízké","cfm","","","851"]
["","","Vytápění","Velmi nízké","cfm","","","851"]
["Rozměry","Jednotka","","Výška","mm","734","734","734"]
["","","","Šířka","mm","974","974","958"]
["","","","Hloubka","mm","401","401","340"]
["Hmotnost","Jednotka","","","kg","57","57","62"]
["Motor ventilátoru","Otáčky","Chlazení","Velmi nízké","ot./min","420","420"]
["","","Vytápění","Velmi nízké","ot./min","420","420"]
["Kompresor","Typ","","","","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CST","-10","-10","-10"]
["","","","Max.","°CST","46","46","46"]
["","Vytápění","Okolí","Min.","° CWB","","","-15"]
["","","","Max.","° CWB","","","24"]
["Hladina akustického tlaku","Chlazení","","Jm.","dBA","46","46","48"]
["","Vytápění","","Jm.","dBA","47","47","48"]
["Chladivo","Typ","","","","R-32","R-32","R-32"]
["","Náplň","","","kg","1.8","1.8","2"]
["","Náplň","","","tCO2Eq","1.22","1.22"]
["","Vliv na globální oteplování (GWP)","","","","675","675","675"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","25","25 (1)","25"]
["","Doplňková náplň chladiva","","","kg/m","0,02 (pro délku potrubí přesahující 30m)","0,02 (pro délku potrubí přesahující 30m)","0,02 (pro délku potrubí přesahující 30m)"]
["","Rozdíl hladin","IU - OU","Max.","m","15.0","15.0","15"]
["","","IU - IU","Max.","m","7.5","7.5","7.5"]
["","Celková délka potrubí","Systém","Skutečná","m","50","50 (2)","50"]
["Standardní příslušenství","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Napájení","Fáze","","","","1~","1~","1~"]
["","Frekvence","","","Hz","50","50","50"]
["","Napětí","","","V","220-240","220-240","220-440"]
["Poznámky","","","","","(1) - Jedna místnost","(1) - Jedna místnost"]
["","","","","","(2) - Pro kombinaci s CVXM-A, FVXM-A – maximální délka potrubí 30 m.","(2) - Pro kombinaci s CVXM-A, FVXM-A – maximální délka potrubí 30 m."]
["Kompresor","Typ","","","","","","Hermeticky utěsněný rotační kompresor"]
["Standardní příslušenství","Příručka pro instalaci","","","","","","1"]
["","Krytka vypouštění","","","","","","3"]
["","Uzávěr vypouštění","","","","","","1"]
["","Sestava reduktoru","","","","","","1"]
["","Sáček se šrouby","","","","","","1"]
["Energetickou účinná řada","","","","","","","A+++ ~ D"]