{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":8,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXS-F"]
[]
[]
[]
[]
["","","","","","4MXS68F3V1B2","4MXS68F3V1B","4MXS68F2V1B"]
["Hladina akustického tlaku","Vytápění","","Jm.","dBA","49","49"]
["","Chlazení","","Jm.","dBA","48","48"]
["Standardní příslušenství","Příručka pro instalaci","","","","1","1"]
["","Uzávěr vypouštění","","","","1","1"]
["","Sestava reduktoru","","","","1","1"]
["Chladivo","Charge","","","TCO2Eq","5.4","5.4"]
["","Vliv na globální oteplování (GWP)","","","","2,087.5","2,087.5"]
["","Náplň","","","kg","2.6","2.6"]
["","Typ","","","","R-410A","R-410A"]
["Provozní rozsah","Chlazení","Okolí","Max.","°CST","46"]
["","","","Min.","°CST","-10"]
["","Vytápění","Okolí","Max.","° CWB","18"]
["","","","Min.","° CWB","-15"]
["Spoje potrubí","Rozdíl hladin","IU - IU","Max.","m","7.5"]
["","","IU - OU","Max.","m","15"]
["","Doplňková náplň chladiva","","","kg/m","0,02 (pro délku potrubí přesahující 30m)"]
["","Celková délka potrubí","Systém","Skutečná","m","60"]
["Kompresor","Typ","","","","Hermeticky utěsněný rotační kompresor"]
["Rozměry","Jednotka","","Šířka","mm","936","936"]
["","","","Hloubka","mm","300","300"]
["","","","Výška","mm","735","735"]
["Hmotnost","Jednotka","","","kg","58","58"]
["Power supply","Fáze","","","","1~","1~"]
["","Frekvence","","","Hz","50","50"]
["","Napětí","","","V","230","230"]
["Poznámky","","","","","(1) - Chlazení: vnitřní teplota 27 °CDB, 19,0 °CWB; venkovní teplota 35 °CST; ekvivalentní délka potrubí: 5m","(1) - Chlazení: vnitřní teplota 27 °CDB, 19,0 °CWB; venkovní teplota 35 °CST; ekvivalentní délka potrubí: 5m"]
["","","","","","(2) - Vytápění: vnitřní teplota 20° CDB; vnější teplota 7° CDB, 6° CWB ekvivalentní délka potrubí chladiva: 5m","(2) - Vytápění: vnitřní teplota 20° CDB; vnější teplota 7° CDB, 6° CWB ekvivalentní délka potrubí chladiva: 5m"]
["","","","","","(3) - Obsahuje fluorované skleníkové plyny","(3) - Obsahuje fluorované skleníkové plyny"]
["Spoje potrubí","Rozdíl hladin","IU - IU","Max.","m","","7.5"]
["","","IU - OU","Max.","m","","15"]
["","Doplňková náplň chladiva","","","kg/m","","0,02 (pro délku potrubí přesahující 30m)"]
["","Celková délka potrubí","Systém","Skutečná","m","","60"]
["Kompresor","Typ","","","","","Hermeticky utěsněný rotační kompresor"]
["Rozměry","Jednotka","","Výška","mm","","","735"]
["","","","Šířka","mm","","","936"]
["","","","Hloubka","mm","","","300"]
["Hmotnost","Jednotka","","","kg","","","58"]
["Kompresor","Typ","","","","","","Hermeticky utěsněný rotační kompresor"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CST","","","-10"]
["","","","Max.","°CST","","","46"]
["","Vytápění","Okolí","Min.","° CWB","","","-15"]
["","","","Max.","° CWB","","","15.5"]
["Hladina akustického tlaku","Chlazení","","Jm.","dBA","","","48"]
["","Vytápění","","Jm.","dBA","","","49"]
["Chladivo","Typ","","","","","","R-410A"]
["","Náplň","","","kg","","","2.6"]
["","Náplň","","","tCO2Eq","","","5.4"]
["","Vliv na globální oteplování (GWP)","","","","","","2087.5"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","","","25"]
["","Doplňková náplň chladiva","","","kg/m","","","0,02 (pro délku potrubí přesahující 30m)"]
["","Rozdíl hladin","IU - OU","Max.","m","","","15"]
["","","IU - IU","Max.","m","","","7.5"]
["","Celková délka potrubí","Systém","Skutečná","m","","","60"]
["Standardní příslušenství","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["","Reducer assembly","","","","","","1"]
["Napájení","Fáze","","","","","","1~"]
["","Frekvence","","","Hz","","","50"]
["","Napětí","","","V","","","230"]