{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MXM-N"]
[]
[]
[]
[]
["","","","","","5MXM90N2V1B (Archived)"]
["Ventilátor","Průtok vzduchu","Chlazení","Velmi nízké","m³/min","24.1"]
["","","Vytápění","Velmi nízké","m³/min","24.1"]
["","","","Velmi nízké","cfm","851"]
["","","Vytápění","Velmi nízké","cfm","851"]
["Rozměry","Jednotka","","Výška","mm","734"]
["","","","Šířka","mm","958"]
["","","","Hloubka","mm","340"]
["Hmotnost","Jednotka","","","kg","68"]
["Compressor","Typ","","","","Hermeticky utěsněný rotační kompresor"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CST","-10"]
["","","","Max.","°CST","46"]
["","Vytápění","Okolí","Min.","° CWB","-15"]
["","","","Max.","° CWB","18"]
["Hladina akustického tlaku","Chlazení","","Jm.","dBA","52"]
["","Vytápění","","Jm.","dBA","52"]
["Chladivo","Typ","","","","R-32"]
["","Náplň","","","kg","2.40"]
["","Náplň","","","tCO2Eq","1.6"]
["","Vliv na globální oteplování (GWP)","","","","675"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","25"]
["","Doplňková náplň chladiva","","","kg/m","0,02 (pro délku potrubí přesahující 30m)"]
["","Rozdíl hladin","IU - OU","Max.","m","15"]
["","","IU - IU","Max.","m","7.5"]
["","Celková délka potrubí","Systém","Skutečná","m","75"]
["Standardní příslušenství","Installation manual","","","","1"]
["","Drain cap","","","","3"]
["","Drain plug","","","","1"]
["","Reducer assembly","","","","1"]
["","Screw bag","","","","1"]
["Napájení","Fáze","","","","1~"]
["","Frekvence","","","Hz","50"]
["","Napětí","","","V","220-240"]