{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":9,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C"]
[]
[]
[]
[]
["","","","","","ABQ71CV1","ABQ100CV1","ABQ125CV1","ABQ140CV1"]
["Standardní příslušenství","Příručka pro instalaci","","","","Příručka pro instalaci"]
["","Manuální ovládání","","","","Manuální ovládání"]
["","Šroub + podložka","","","","Šroub + podložka"]
["","Bezdrátové dálkové ovládání","","","","Bezdrátové dálkové ovládání"]
["","Mřížka zámku krytu","","","","Mřížka zámku krytu"]
["","Baterie","","","","Baterie"]
["Piping connections","Liquid","","OD","mm","9.52"]
["","Plyn","","OD","mm","15.88"]
["","Vypouštění","","","","19.05"]
["Vstup napájení","Chlazení","","Jm.","kW","0.128"]
["","Vytápění","","Jm.","kW","0.128"]
["Hladina akustického výkonu","Chlazení","","","dBA","64"]
["","Vytápění","","","dBA","64"]
["Rozměry","Jednotka","","Width","mm","600"]
["","","","Depth","mm","1,007"]
["","","","Výška","mm","285"]
["Opláštění","Materiál","","","","Pozinkovaná ocel"]
["Hmotnost","Jednotka","","","kg","35"]
["Ventilátor","Vnější statický tlak","","Vysoký","Pa","90"]
["","","","Jmen.","Pa","77"]
["","","","Nízký","Pa","64"]
["Power supply","Fáze","","","","1~"]
["","Frekvence","","","Hz","50"]
["","Označení","","","","V1"]
["","Napětí","","","V","220-240"]
["Vstup napájení","Vytápění","","Jm.","kW","","0.109"]
["","Chlazení","","Jm.","kW","","0.109"]
["Ventilátor","Vnější statický tlak","","Vysoký","Pa","","70","150","150"]
["","","","Nízký","Pa","","45","111","92"]
["Opláštění","Materiál","","","","","Pozinkovaná ocel"]
["Rozměry","Jednotka","","Výška","mm","","378","378","378"]
["","","","Šířka","mm","","541","1300","1500"]
["","","","Hloubka","mm","","1045","541","541"]
["Hmotnost","Jednotka","","","kg","","44","50","56"]
["Ventilátor","Průtok vzduchu","Chlazení","Vysoké","m³/min","","22.7","40.5","48.7"]
["","","","Jm.","m³/min","","20.5","37","44"]
["","","","Nízký","m³/min","","18.3","34.8","37.9"]
["","","Vytápění","Vysoké","m³/min","","22.7","40.5","48.7"]
["","","","Jm.","m³/min","","20.5","37.4","43.9"]
["","","","Nízký","m³/min","","18.3","34.8","37.9"]
["","Vnější statický tlak","","Jmen.","Pa","","57","128","122"]
["Hladina akustického výkonu","Chlazení","","","dBA","","60","72","73"]
["","Vytápění","","","dBA","","60","72","73"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","","41","53","55"]
["","","","Jm.","dBA","","38"]
["","","","Nízký","dBA","","36","50","50"]
["","Vytápění","","Vysoké","dBA","","41","53","55"]
["","","","Jm.","dBA","","38"]
["","","","Nízký","dBA","","36","50","50"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","","9.52","9.52","9.52"]
["","Plyn","","Vnější průměr","mm","","15.88","15.9","15.9"]
["","Odvod kondenzátu","","","","","19.05"]
["Standardní příslušenství","Installation manual","","","","","Installation manual"]
["","Wireless remote control","","","","","Wireless remote control"]
["","Cover lock grill","","","","","Cover lock grill"]
["","Battery","","","","","Battery"]
["","Screw+Washer","","","","","Screw+Washer"]
["","Operation manual","","","","","Operation manual"]
["Napájení","Fáze","","","","","1~"]
["","Frekvence","","","Hz","","50"]
["","Napětí","","","V","","220-240"]
["Chladicí výkon","Celkový výkon","","Jm.","kW","","","12.10","13.00"]
["Topný výkon","Celkový výkon","","Jmen.","kW","","","13.5","15.5"]
["Opláštění","Barva","","","","","","Galvanizovaná ocelová deska / nelakovaná","Galvanizovaná ocelová deska / nelakovaná"]
["Ventilátor","Průtok vzduchu","Chlazení","Střední","m³/min","","","37","44"]
["","","Vytápění","Střední","m³/min","","","37.4","43.9"]
["Hladina akustického tlaku","Chlazení","","Střední","dBA","","","52","53"]
["","Vytápění","","Střední","dBA","","","52","53"]
["Řídicí systémy","Infračervené dálkové ovládání","","","","","","ARCWLA","ARCWLA"]