{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-C / AZQS-B(8)V1"]
[]
[]
[]
[]
["","","","","ACQ71CV1 / AZQS71B2V1B","ACQ100CV1 / AZQS100B8V1B","ACQ125CV1 / AZQS125B8V1B"]
["Chladicí výkon","Jm.","","kW","6.8","9.5","12.1"]
["Prostorové chlazení","SEER","","","4.65","4.65"]
["","Roční spotřeba energie","","kWh/rok","512","716"]
["","Kapacita","Pnávrh","kW","6.80","9.50"]
["","Třída energetické úspornosti","","","B","B"]
["Prostorové vytápění (průměrné klima)","Výkon","Pnávrh","kW","6.33","7.60"]
["","SCOP/A","","","3.80","3.80"]
["","Třída energetické účinnosti","","","A","A"]
["","Roční spotřeba energie","","kWh/rok","2,332","2,800"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","1,025","1,480","2,010"]
["","EER","","","3.31","3.21","3.01"]
["","COP","","","3.61","3.61","3.41"]
["","Směrnice o energetických štítcích","Chlazení","","B","A"]
["","","Vytápění","","A","A"]
["Topný výkon","Jm.","","kW","7.50","10.80","13.5"]
["Poznámky","","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]
["","","","","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]