{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-A / AZQS-B(8)V1"]
[]
[]
[]
[]
["","","","","ADEQ100A7VEB / AZQS100B8V1B","ADEQ125A7VEB / AZQS125B8V1B","ADEQ71A7VEB / AZQS71B2V1B (Archived)"]
["Chladicí výkon","Jm.","","kW","9.5","12.1","6.8"]
["Prostorové chlazení","SEER","","","4.81","","4.81"]
["","Roční spotřeba energie","","kWh/rok","692","","494.77"]
["","Kapacita","Pnávrh","kW","9.50","","6.80"]
["","Třída energetické úspornosti","","","B","","B"]
["Prostorové vytápění (průměrné klima)","Výkon","Pnávrh","kW","7.60","","6.00"]
["","SCOP/A","","","3.81","","3.81"]
["","Třída energetické účinnosti","","","A","","A"]
["","Roční spotřeba energie","","kWh/rok","2,793","","2,205.68"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","1,480","2,010","1,060"]
["","EER","","","3.21","3.01","3.21"]
["","COP","","","3.61","3.45","3.61"]
["","Směrnice oenergetických štítcích","Chlazení","","A","","A"]
["","","Vytápění","","A","","A"]
["Topný výkon","Jm.","","kW","10.8","13.50","7.50"]
["Poznámky","","","","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU","(1) - EER/COP podle Eurovent 2012, pro použití pouze mimo státy EU"]
["","","","","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení","(2) - Jmenovitá účinnost: chlazení při 35°/27° jmenovité zatížení, vytápění při 7°/20° jmenovité zatížení"]