{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":10,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-C"]
[]
[]
[]
[]
["","","","","ADEQ35C2VEB","ADEQ50C2VEB","ADEQ60C2VEB","ADEQ71C2VEB","ADEQ100C2VEB","ADEQ125C2VEB"]
["Hladina akustického tlaku","Vytápění","Vysoké","dBA","37","37","31","31","36","38"]
["","","Jm.","dBA","37","37","31","31","36","38"]
["","","Střední","dBA","34","34","28","28","33","35"]
["","","Nízký","dBA","29","29","25","25","30","32"]
["","Chlazení","Střední","dBA","32","32","28","28","32","35"]
["","","Nízký","dBA","29","29","25","25","30","32"]
["","","Vysoké","dBA","35","35","30","30","34","37"]
["","","Jm.","dBA","35","35","30","30","34","37"]
["Standardní příslušenství","Manuální ovládání","","","1","1","1","1","1","1"]
["","Příručka pro instalaci","","","1","1","1","1","1","1"]
["","Drenážní hadice","","","1","1","1","1","1","1"]
["","Kovová svorka na drenážní hadici","","","1","1","1","1","1","1"]
["","Podložka pro konzoli závěsu","","","8","8","8","8","8","8"]
["","Šrouby","","","40","40","40","40","40","40"]
["","Izolace pro upevnění","","","2","2","2","2","2","2"]
["","Těsnicí podložky","","","5","5","5","5","5","5"]
["","Svorky","","","4","4","4","4","4","4"]
["Chladivo","Vliv na globální oteplování (GWP)","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["Chladicí výkon","Celkový výkon","Jm.","kW","","","","","","12.10"]
["Piping connections","Kapalina","Vnější průměr","mm","6.35","6.35","6.35","9.52","9.52","9.52"]
["","Plyn","OD","mm","9.52","12.7","12.7","15.9","15.9","15.9"]
["","Drain","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Hladina akustického výkonu","Chlazení","","dBA","60","60","56","56","58","62"]
["Rozměry","Jednotka","Šířka","mm","700","700","1,000","1,000","1,400","1,400"]
["","","Hloubka","mm","800","800","800","800","800","800"]
["","","Výška","mm","245","245","245","245","245","245"]
["Opláštění","Materiál","","","Pozinkovaný ocelový plech","Pozinkovaný ocelový plech","Pozinkovaný ocelový plech","Pozinkovaný ocelový plech","Pozinkovaný ocelový plech","Pozinkovaný ocelový plech"]
["","Barva","","","Nelakovaný","Nelakovaný","Nelakovaný","Nelakovaný","Nelakovaný","Nelakovaný"]
["Hmotnost","Jednotka","","kg","28.0","28.0","35.0","35","46","46"]
["Ventilátor","Vnější statický tlak","Vysoký","Pa","150","150","150","150","150","150"]
["","","Jmen.","Pa","30","30","30","30","40","50"]
["Topný výkon","Celkový výkon","Jmen.","kW","","","","","","13.5"]
["Power supply","Fáze","","","1~","1~","1~","1~","1~","1~"]
["","Frekvence","","Hz","50","50","50","50","50","50"]
["","Napětí","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Poznámky","","","","(1) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer.","(1) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer.","(1) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer.","(1) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer.","(1) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer.","(1) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer."]