{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXP-N"]
[]
[]
[]
[]
["","","","","","ARXP25N5V1B","ARXP35N5V1B"]
["Rozměry","Jednotka","","Výška","mm","556","556"]
["","","","Šířka","mm","740","740"]
["","","","Hloubka","mm","343","343"]
["Hmotnost","Jednotka","","","kg","24","24"]
["Kompresor","Typ","","","","Hermeticky utěsněný rotační kompresor","Hermeticky utěsněný rotační kompresor"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CST","-10","-10"]
["","","","Max.","°CST","48","48"]
["","Vytápění","Okolí","Min.","° CWB","-15","-15"]
["","","","Max.","° CWB","18","18"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","46","48"]
["","Vytápění","","Vysoké","dBA","47","48"]
["Chladivo","Typ","","","","R-32","R-32"]
["","Náplň","","","kg","0.55","0.70"]
["","Náplň","","","tCO2Eq","0.37","0.48"]
["","Vliv na globální oteplování (GWP)","","","","675.0","675.0"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","20","20"]
["","Doplňková náplň chladiva","","","kg/m","0,02 (pro délku potrubí přesahující 10m)","0,02 (pro délku potrubí přesahující 10m)"]
["","Rozdíl hladin","IU - OU","Max.","m","12","12"]
["Standardní příslušenství","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","Drain plug","","","","1","1"]
["Napájení","Fáze","","","","1~","1~"]
["","Frekvence","","","Hz","50","50"]
["","Napětí","","","V","220-240","220-240"]