{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L3"]
[]
[]
[]
[]
["","","","","","ARXS25L3V1B","ARXS35L3V1B"]
["Hladina akustického tlaku","Vytápění","","Vysoké","dBA","","48"]
["","","","Nízký","dBA","","45"]
["Standardní příslušenství","1","","","","","550"]
["Chladivo","Náplň","","","kg","","2.5"]
["","Typ","","","","","1.2"]
["Ventilátor","Průtok vzduchu","Chlazení","Velmi nízké","m³/min","","30.1"]
["","","","Velmi nízké","cfm","","1,063"]
["Motor ventilátoru","Otáčky","Chlazení","Velmi nízké","ot/min","","740"]
["","","Vytápění","Velmi nízké","ot/min","","-15"]
["Provozní rozsah","Vytápění","Okolí","Min.","° CWB","","20"]
["","","","Max.","° CWB","","10"]
["Hladina akustického tlaku","Chlazení","","Nízký","dBA","","44"]
["","","","Vysoké","dBA","","48"]
["Kompresor","Type","","","","","Hermeticky utěsněný rotační kompresor"]
["Rozměry","Jednotka","","Šířka","mm","","285"]
["","","","Hloubka","mm","","612"]
["","","","Výška","mm","","765"]
["Hmotnost","Jednotka","","","kg","","34"]
["Ventilátor","Průtok vzduchu","Vytápění","Velmi nízké","cfm","","904"]
["","","","Velmi nízké","m³/min","","25.6"]
["Power supply","Phase","","","","","1~"]
["","Frekvence","","","Hz","","50"]
["","Napětí","","","V","","220-240"]
["Poznámky","","","","","(1) - 220 V","(1) - Obsahuje fluorované skleníkové plyny"]
["","","","","","(2) - 230V","(2) - 220 V"]
["","","","","","(3) - 240 V","(3) - 230V"]
["","","","","","","(4) - 240 V"]
["Ventilátor","Průtok vzduchu","Chlazení","Velmi nízké","m³/min","30.1"]
["","","Vytápění","Velmi nízké","m³/min","25.6"]
["","","","Velmi nízké","cfm","1063"]
["","","Vytápění","Velmi nízké","cfm","904"]
["Rozměry","Jednotka","","Výška","mm","550"]
["","","","Šířka","mm","765"]
["","","","Hloubka","mm","285"]
["Hmotnost","Jednotka","","","kg","34"]
["Motor ventilátoru","Otáčky","Chlazení","Velmi nízké","ot/min","780"]
["","","Vytápění","Velmi nízké","ot/min","740"]
["Kompresor","Typ","","","","Hermeticky utěsněný rotační kompresor"]
["Provozní rozsah","Chlazení","Okolí","Min.","°CST","10"]
["","","","Max.","°CST","46"]
["","Vytápění","Okolí","Min.","° CWB","-15"]
["","","","Max.","° CWB","18"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","46"]
["","Vytápění","","Vysoké","dBA","47"]
["","","","Nízký","dBA","44"]
["Chladivo","Typ","","","","R-410A"]
["","Náplň","","","kg","1.0"]
["","Náplň","","","tCO2Eq","2.1"]
["","Vliv na globální oteplování (GWP)","","","","2087.5"]
["Spoje potrubí","Délka potrubí","Max.","OU - IU","m","20"]
["","Doplňková náplň chladiva","","","kg/m","0,02 (pro délku potrubí přesahující 10m)"]
["","Rozdíl hladin","IU - OU","Max.","m","15"]
["Standardní příslušenství","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain plug","","","","1"]
["Napájení","Fáze","","","","1~"]
["","Frekvence","","","Hz","50"]
["","Napětí","","","V","220-240"]