{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":86,"n_cols":10,"rows_kept":86,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATX-KV"]
[]
[]
[]
[]
["","","","","","ATX20K5V1B","ATX25K2V1B","ATX25K5V1B","ATX35K5V1B","ATX35K2V1B (Archived)"]
["Hladina akustického tlaku","Vytápění","","Vysoké","dBA","","","","","43"]
["","","","Střední","dBA","","","","","35"]
["","","","Tichý provoz","dBA","","","","","26"]
["","","","Nízký","dBA","","","","","29"]
["","Chlazení","","Střední","dBA","","","","","34"]
["","","","Tichý provoz","dBA","","","","","20"]
["","","","Nízký","dBA","","","","","27"]
["","","","Vysoké","dBA","","","","","43"]
["Standardní příslušenství","Příručka pro instalaci","","","","","","","","1"]
["","Manuální ovládání","","","","","","","","1"]
["","Infračervené dálkové ovládání","","","","","","","","1"]
["","Baterie AA","","","","","","","","2"]
["","Držák dálkového ovládání","","","","","","","","1"]
["","Montážní deska","","","","","","","","1"]
["","Fotokatalytický filtr s apatitem titanu pro čištění vzduchu","","","","","","","","2"]
["","Upevňovací šrouby vnitřní jednotky","","","","","","","","2"]
["Řídicí systémy","Wired remote control","","","","","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","","","","","ARC480A11"]
["Spoje potrubí","Kapalina","","Vnější průměr","mm","","","","","6.35"]
["","Plyn","","Vnější průměr","mm","","","","","9.50"]
["","Vypouštění","","","","","","","","18"]
["Příkon","Chlazení","","Jm.","kW","","","","","0.024"]
["","Vytápění","","Jm.","kW","","","","","0.029"]
["Sound power level","Chlazení","","","dBA","","","","","58"]
["","Vytápění","","","dBA","","","","","58"]
["Rozměry","Jednotka","","Šířka","mm","","","","","770"]
["","","","Hloubka","mm","","","","","225"]
["","","","Výška","mm","","","","","286"]
["Opláštění","Barva","","","","","","","","Bílý"]
["Hmotnost","Jednotka","","","kg","","","","","9.0"]
["Power supply","Fáze","","","","","","","","1~"]
["","Frekvence","","","Hz","","","","","50"]
["","Označení","","","","","","","","V1"]
["","Napětí","","","V","","","","","220-240"]
["Poznámky","","","","","","","","","(1) - SL: Luftstrømmens hastighedsindstillings lydløse ventilatorniveau"]
["Vstup napájení","Chlazení","","Jm.","kW","0.018","0.02","0.02","0.024"]
["","Vytápění","","Jm.","kW","0.022","0.023","0.023","0.029"]
["Opláštění","Barva","","","","Bílá","Bílá","Bílá","Bílá"]
["Rozměry","Jednotka","","Výška","mm","286","286","286","286"]
["","","","Šířka","mm","770","770","770","770"]
["","","","Hloubka","mm","225","225","225","225"]
["Hmotnost","Jednotka","","","kg","8.5","8.5","8.5","9"]
["Ventilátor","Průtok vzduchu","Chlazení","Vysoké","m³/min","9.9","10.4","10.4","11.8"]
["","","","Střední","m³/min","7.8","8","8","8.2"]
["","","","Nízký","m³/min","5.8","6.1","6.1","6.3"]
["","","","Tichý provoz","m³/min","4.8","4.8","4.8","4.9"]
["","","Vytápění","Vysoké","m³/min","10.9","11.1","11.1","12.8"]
["","","","Střední","m³/min","8.5","8.5","8.5","8.5"]
["","","","Nízký","m³/min","6.4","6.7","6.7","6.9"]
["","","","Tichý provoz","m³/min","5.2","5.2","5.2","5.2"]
["Hladina akustického výkonu","Chlazení","","","dBA","55","55","55","58"]
["","Vytápění","","","dBA","55","55","55","58"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","39","40","40","43"]
["","","","Střední","dBA","33","33","33","34"]
["","","","Nízký","dBA","25","26","26","27"]
["","","","Tichý provoz","dBA","20","20","20","20"]
["","Vytápění","","Vysoké","dBA","39","40","40","43"]
["","","","Střední","dBA","34","34","34","35"]
["","","","Nízký","dBA","28","28","28","29"]
["","","","Tichý provoz","dBA","23","23","23","26"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","6.35","6.35","6.35","6.35"]
["","Plyn","","Vnější průměr","mm","9.5","9.5","9.5","9.5"]
["","Odvod kondenzátu","","","","18","18","18","18"]
["Řídicí systémy","Infrared remote control","","","","ARC480A11","","","ARC480A11"]
["Řídicí systémy","Kabelové dálkové ovládání","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standardní příslušenství","Installation manual","","","","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","","2","2"]
["","Operation manual","","","","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["Napájení","Označení","","","","V1","V1","V1","V1"]
["","Fáze","","","","1~","1~","1~","1~"]
["","Frekvence","","","Hz","50","50","50","50"]
["","Napětí","","","V","220-240","220-240","220-240","220-240"]
["Řídicí systémy","Infračervené dálkové ovládání","","","","","ARC480A11","ARC480A11"]
["Standardní příslušenství","AA dry-cell batteries","","","","","2"]
["","Titanium apatite photocatalytic air purification filter","","","","","2"]