{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":87,"n_cols":11,"rows_kept":87,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-A"]
[]
[]
[]
[]
["","","","","","ATXF20A5V1B","ATXF50A2V1B","ATXF60A2V1B","ATXF71A2V1B","ATXF25A5V1B (Archived)","ATXF35A5V1B (Archived)"]
["Hladina akustického tlaku","Vytápění","","Vysoké","dBA","40","42","44","45"]
["","","","Střední","dBA","34","38","40","41"]
["","","","Tichý provoz","dBA","21","30","32","33"]
["","","","Nízký","dBA","28","33","35","36"]
["","Chlazení","","Střední","dBA","33","39","41","42"]
["","","","Tichý provoz","dBA","20","31","33","34"]
["","","","Nízký","dBA","26","34","36","37"]
["","","","Vysoké","dBA","40","43","45","46"]
["Standardní příslušenství","Příručka pro instalaci","","","","1","1","1","1"]
["","Manuální ovládání","","","","1","1","1","1"]
["","Infračervené dálkové ovládání","","","","1","1","1","1"]
["","Baterie AAA","","","","2","2","2","2"]
["","Držák dálkového ovládání","","","","1","1","1","1"]
["","Montážní deska","","","","1","1","1","1"]
["","Upevňovací šrouby vnitřní jednotky","","","","2","2","2","2"]
["Řídicí systémy","Wired remote control","","","","BRC944B2, BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","6.35","6.35","6.35","6.35"]
["","Plyn","","Vnější průměr","mm","9.50","12.7","12.7","12.7"]
["","Vypouštění","","","","18","18","18","18"]
["Vstup napájení","Chlazení","","Jm.","kW","0.019","0.029","0.032","0.032"]
["","Vytápění","","Jm.","kW","0.020","0.032","0.035","0.035"]
["Sound power level","Chlazení","","","dBA","55","59","60","62"]
["","Vytápění","","","dBA","55","61","62","62"]
["Rozměry","Jednotka","","Šířka","mm","770","990","990","990"]
["","","","Hloubka","mm","225","263","263","263"]
["","","","Výška","mm","286","295","295","295"]
["Opláštění","Barva","","","","Bílý","Bílý","Bílý","Bílý"]
["Hmotnost","Jednotka","","","kg","8.50","13.5","13.5","13.5"]
["Ventilátor","Průtok vzduchu","Vytápění","Vysoké","m³/min","10.3","17.3","17.9","17.9"]
["","","","Nízký","m³/min","6.7","12.2","12.8","12.8"]
["","","","Střední","m³/min","8.6","14.8","15.8","15.8"]
["","","","Tichý provoz","m³/min","5.3","10.7","11.3","11.3"]
["","","Chlazení","Nízký","m³/min","6.1","11.9","12.2","12.2"]
["","","","Střední","m³/min","8.1","14.4","14.8","14.8"]
["","","","Vysoké","m³/min","10.1","16.8","17.3","17.3"]
["","","","Tichý provoz","m³/min","4.4","10.5","10.7","10.7"]
["Power supply","Fáze","","","","1~","1~","1~","1~"]
["","Frekvence","","","Hz","50","50","50","50"]
["","Označení","","","","","V1","V1","V1"]
["","Napětí","","","V","220-240","220-240","220-240","220-240"]
["Vstup napájení","Chlazení","","Jm.","kW","","","","","0.019","0.032"]
["","Vytápění","","Jm.","kW","","","","","0.02","0.032"]
["Opláštění","Barva","","","","","","","","Bílá","Bílá"]
["Rozměry","Jednotka","","Výška","mm","","","","","286","286"]
["","","","Šířka","mm","","","","","770","770"]
["","","","Hloubka","mm","","","","","225","225"]
["Hmotnost","Jednotka","","","kg","","","","","8.5","9"]
["Ventilátor","Průtok vzduchu","Chlazení","Vysoké","m³/min","","","","","10.1","11.5"]
["","","","Střední","m³/min","","","","","8.1","8.3"]
["","","","Nízký","m³/min","","","","","6.1","6.3"]
["","","","Tichý provoz","m³/min","","","","","4.4","4.5"]
["","","Vytápění","Vysoké","m³/min","","","","","10.3","11.5"]
["","","","Střední","m³/min","","","","","8.6","9"]
["","","","Nízký","m³/min","","","","","6.7","7"]
["","","","Tichý provoz","m³/min","","","","","5.3","5.3"]
["Hladina akustického výkonu","Chlazení","","","dBA","","","","","55","58"]
["","Vytápění","","","dBA","","","","","55","58"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","","","","","40","43"]
["","","","Střední","dBA","","","","","33","34"]
["","","","Nízký","dBA","","","","","26","27"]
["","","","Tichý provoz","dBA","","","","","20","20"]
["","Vytápění","","Vysoké","dBA","","","","","40","40"]
["","","","Střední","dBA","","","","","34","35"]
["","","","Nízký","dBA","","","","","28","29"]
["","","","Tichý provoz","dBA","","","","","21","21"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","","","","","6.35","6.35"]
["","Plyn","","Vnější průměr","mm","","","","","9.5","9.5"]
["","Odvod kondenzátu","","","","","","","","18","18"]
["Řídicí systémy","Infračervené dálkové ovládání","","","","","","","","ARC470A1","ARC470A1"]
["","Kabelové dálkové ovládání","","","","","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standardní příslušenství","Installation manual","","","","","","","","1","1"]
["","AAA dry-cell batteries","","","","","","","","2","2"]
["","Operation manual","","","","","","","","1","1"]
["","Indoor unit fixing screws","","","","","","","","2","2"]
["","Infrared remote control","","","","","","","","1","1"]
["","Mounting plate","","","","","","","","1","1"]
["","Remote control holder","","","","","","","","1","1"]
["Napájení","Fáze","","","","","","","","1~","1~"]
["","Frekvence","","","Hz","","","","","50","50"]
["","Napětí","","","V","","","","","220-240","220-240"]