{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":80,"n_cols":9,"rows_kept":80,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-C"]
[]
[]
[]
[]
["","","","","","ATXF20C5V1B","ATXF25C5V1B","ATXF35C5V1B","ATXF42C5V1B"]
["Hladina akustického tlaku","Vytápění","","Vysoké","dBA","39.0","40.0","","44.0"]
["","","","Střední","dBA","34.0","34.0","","34.0"]
["","","","Tichý provoz","dBA","21.0","21.0","","22.0"]
["","","","Nízký","dBA","28.0","28.0","","28.0"]
["","Chlazení","","Střední","dBA","33.0","33.0","","36.0"]
["","","","Tichý provoz","dBA","20.0","20.0","","22.0"]
["","","","Nízký","dBA","25.0","26.0","","30.0"]
["","","","Vysoké","dBA","39.0","40.0","","45.0"]
["Standardní příslušenství","Příručka pro instalaci","","","","1","1","","1"]
["","Manuální ovládání","","","","1","1","","1"]
["","Baterie","","","","1","1","","1"]
["","Infračervené dálkové ovládání","","","","1","1","","1"]
["","Baterie AAA","","","","2","2","","2"]
["","Držák dálkového ovládání","","","","1","1","","1"]
["","Montážní deska","","","","1","1","","1"]
["","Upevňovací šrouby vnitřní jednotky","","","","2","2","","2"]
["Řídicí systémy","Wired remote control","","","","BRC073A1","BRC073A1","","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1","","ARC470A1"]
["Spoje potrubí","Liquid","","OD","mm","6.35","6.35","","6.35"]
["","Plyn","","OD","mm","9.50","9.50","","9.50"]
["","Vypouštění","","","","18","18","","18"]
["Příkon","Chlazení","","Jm.","kW","0.023","0.023","","0.040"]
["","Vytápění","","Jm.","kW","0.023","0.023","","0.040"]
["Hladina akustického výkonu","Chlazení","","","dBA","53.0","54.0","","59.0"]
["","Vytápění","","","dBA","55.0","55.0","","59.0"]
["Rozměry","Jednotka","","Šířka","mm","770","770","","770"]
["","","","Hloubka","mm","225","225","","225"]
["","","","Výška","mm","286","286","","286"]
["Casing","Barva","","","","Bílý","Bílý","","Bílý"]
["Hmotnost","Jednotka","","","kg","8.00","8.00","","9.00"]
["Power supply","Fáze","","","","1~","1~","","1~"]
["","Frekvence","","","Hz","50","50","","50"]
["","Napětí","","","V","220-440","220-440","","220-440"]
["Vstup napájení","Chlazení","","Jm.","kW","","","0.029"]
["","Vytápění","","Jm.","kW","","","0.029"]
["Opláštění","Barva","","","","","","Bílá"]
["Rozměry","Jednotka","","Výška","mm","","","286"]
["","","","Šířka","mm","","","770"]
["","","","Hloubka","mm","","","225"]
["Hmotnost","Jednotka","","","kg","","","8.5"]
["Ventilátor","Průtok vzduchu","Chlazení","Vysoké","m³/min","","","11.8"]
["","","","Střední","m³/min","","","8"]
["","","","Nízký","m³/min","","","6.4"]
["","","","Tichý provoz","m³/min","","","4.4"]
["","","Vytápění","Vysoké","m³/min","","","11.9"]
["","","","Střední","m³/min","","","8.6"]
["","","","Nízký","m³/min","","","6.5"]
["","","","Tichý provoz","m³/min","","","5.3"]
["Hladina akustického výkonu","Chlazení","","","dBA","","","54"]
["","Vytápění","","","dBA","","","56"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","","","43"]
["","","","Střední","dBA","","","34"]
["","","","Nízký","dBA","","","27"]
["","","","Tichý provoz","dBA","","","20"]
["","Vytápění","","Vysoké","dBA","","","40"]
["","","","Střední","dBA","","","35"]
["","","","Nízký","dBA","","","29"]
["","","","Tichý provoz","dBA","","","21"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","","","6.35"]
["","Plyn","","Vnější průměr","mm","","","9.5"]
["","Odvod kondenzátu","","","","","","18"]
["Řídicí systémy","Infračervené dálkové ovládání","","","","","","ARC470A1"]
["","Kabelové dálkové ovládání","","","","","","BRC073A1"]
["Standardní příslušenství","Installation manual","","","","","","1"]
["","AAA dry-cell batteries","","","","","","2"]
["","Operation manual","","","","","","1"]
["","Batteries","","","","","","1"]
["","Indoor unit fixing screws","","","","","","2"]
["","Infrared remote control","","","","","","1"]
["","Mounting plate","","","","","","1"]
["","Remote control holder","","","","","","1"]
["Napájení","Fáze","","","","","","1~"]
["","Frekvence","","","Hz","","","50"]
["","Napětí","","","V","","","220-440"]