{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-F / ARXF-A"]
[]
[]
[]
[]
["","","","","ATXF50F5V1B / ARXF50A5V1B"]
["Outdoor unit","","","","ARXF50A5V1B"]
["Chladicí výkon","Min.","","kW","1.7"]
["","Jm.","","kW","5"]
["","Max.","","kW","6"]
["Topný výkon","Min.","","kW","1.7"]
["","Jm.","","kW","6"]
["","Max.","","kW","7.7"]
["Jmenovitá účinnost","EER","","","3.3"]
["","COP","","","3.71"]
["","Roční spotřeba energie","","kWh","283"]
["","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Chlazení","","A"]
["","","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Vytápění","","A"]
["Prostorové chlazení","Třída energetické úspornosti","","","A++"]
["","Kapacita","Pnávrh","kW","5"]
["","SEER","","","6.18"]
["","Roční spotřeba energie","","kWh/r","283"]
["Prostorové vytápění (průměrné klima)","Třída energetické účinnosti","","","A+"]
["","Výkon","Pnávrh","kW","4.6"]
["","SCOP/A","","","4.03"]
["","Topný výkon Pdh při -10°","","kW","4.06"]
["","Roční spotřeba energie","","kWh/r","1598"]
["Poznámky","","","","(1) - Jmenovité chladící výkony jsou založeny na: vnitřní teplota: 27 °CST, 19 °CMT, venkovní teplota: 35 °CST, ekvivalentní délka potrubí chladiva: 5 m, rozdíl úrovní: 0 m. Data pro řadu s vysokou účinností, certifikováno Eurovent"]
["","","","","(2) - Jmenovité topné výkony jsou založeny na: vnitřní teplota: 20 °CST, venkovní teplota: 7 °CST, 6 °CMT, ekvivalentní délka potrubí chladiva: 5 m, rozdíl úrovní: 0 m. Data pro řadu se standardní účinností"]
["","","","","(3) - Údaje o elektrickém systému najdete v samostatném výkresu"]