{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-F"]
[]
[]
[]
[]
["","","","","","ATXF50F5V1B"]
["Vstup napájení","Chlazení","","Jm.","kW","0.04"]
["","Vytápění","","Jm.","kW","0.04"]
["Opláštění","Barva","","","","Bílá"]
["Rozměry","Jednotka","","Výška","mm","286"]
["","","","Šířka","mm","770"]
["","","","Hloubka","mm","225"]
["Hmotnost","Jednotka","","","kg","9"]
["Ventilátor","Průtok vzduchu","Chlazení","Vysoké","m³/min","12.6"]
["","","","Střední","m³/min","9"]
["","","","Nízký","m³/min","7.2"]
["","","","Tichý provoz","m³/min","6.4"]
["","","Vytápění","Vysoké","m³/min","12.8"]
["","","","Střední","m³/min","9.6"]
["","","","Nízký","m³/min","7.2"]
["","","","Tichý provoz","m³/min","6.4"]
["Hladina akustického výkonu","Chlazení","","","dBA","59"]
["","Vytápění","","","dBA","59"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","45"]
["","","","Střední","dBA","39"]
["","","","Nízký","dBA","34"]
["","","","Tichý provoz","dBA","31"]
["","Vytápění","","Vysoké","dBA","44"]
["","","","Střední","dBA","38"]
["","","","Nízký","dBA","33"]
["","","","Tichý provoz","dBA","30"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","6"]
["","Plyn","","Vnější průměr","mm","12.7"]
["","Odvod kondenzátu","","","","18"]
["Řídicí systémy","Infračervené dálkové ovládání","","","","ARC480A93"]
["","Kabelové dálkové ovládání","","","","BRC073A1"]
["Standardní příslušenství","ATXF50F5V1B","","","","1"]
["","Installation manual","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Indoor unit fixing screws","","","","2"]
["","Infrared remote control","","","","1"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["Napájení","Fáze","","","","1~"]
["","Frekvence","","","Hz","50"]
["","Napětí","","","V","220-440"]
["Poznámky","","","","","(1) - Chlazení: vnitřní teplota 27° CDB, 19° CWB; vnější teplota 35 °CST; ekvivalentní délka potrubí: 5m; rozdíl úrovně: 0m"]
["","","","","","(2) - Vytápění: vnitřní teplota 20° CDB; vnější teplota 7° CDB, 6° CWB ekvivalentní délka potrubí chladiva: 5 m (vodorovné)"]
["","","","","","(3) - Údaje o elektrickém systému najdete v samostatném výkresu"]