{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":8,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-R / ARXM-R9"]
[]
[]
[]
[]
["","","","","ATXM25R2V1B / ARXM25R5V1B9","ATXM25R5V1B / ARXM25R5V1B9","ATXM35R2V1B / ARXM35R5V1B9","ATXM35R5V1B / ARXM35R5V1B9"]
["Chladicí výkon","Min.","","kW","","","1.40"]
["","Max.","","kW","","","4.00"]
["","Jm.","","kW","","","3.40"]
["Jmenovitá účinnost","Roční spotřeba energie","","kWh","","","402"]
["","EER","","","","","4.23"]
["","COP","","","","","4.04"]
["","Směrnice oenergetických štítcích","Chlazení","","","","A"]
["","","Vytápění","","","","A"]
["Topný výkon","Jm.","","kW","","","4.00"]
["","Min.","","kW","","","1.40"]
["","Max.","","kW","","","5.20"]
["Poznámky","","","","","","(1) - Viz samostatný výkres s provozním rozsahem"]
["","","","","","","(2) - Údaje o elektrickém systému najdete v samostatném výkresu"]
["","","","","","","(3) - Jmenovité chladicí výkony vycházejí z těchto podmínek: vnitřní teplota: 27°CDB, 19°CWB, venkovní teplota: 35 °CDB, ekvivalentní délka potrubí s chladivem: 5 m, rozdíl úrovní: 0 m."]
["","","","","","","(4) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]
["Chladicí výkon","Min.","","kW","1.30","1.30","","1.40"]
["","Jm.","","kW","2.50","2.50","","3.40"]
["","Max.","","kW","3.20","3.20","","4.00"]
["Topný výkon","Min.","","kW","1.30","1.30","","1.40"]
["","Jm.","","kW","2.80","2.80","","4.00"]
["","Max.","","kW","4.70","4.70","","5.20"]
["Jmenovitá účinnost","EER","","","4.50","4.50","","4.23"]
["","COP","","","5.00","5.00","","4.04"]
["","Roční spotřeba energie","","kWh","278","278","","402"]
["","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Chlazení","","A","A","","A"]
["","","Jmenovitá účinnost-=-Směrnice o&nbsp;energetických štítcích-=-Vytápění","","A","A","","A"]
["Prostorové chlazení","Třída energetické úspornosti","","","A+++","A+++","","A+++"]
["","Kapacita","Pnávrh","kW","2.50","2.50","","3.40"]
["","SEER","","","8.55","8.55","","8.55"]
["","Roční spotřeba energie","","kWh/a","102","102","","139"]
["Prostorové vytápění (průměrné klima)","Třída energetické účinnosti","","","A+++","A+++","","A+++"]
["","Výkon","Pnávrh","kW","2.40","2.40","","2.50"]
["","SCOP/A","","","5.10","5.10","","5.10"]
["","Topný výkon Pdh při -10°","","kW","2.30","2.30","","2.35"]
["","Roční spotřeba energie","","kWh/a","659","659","","686"]
["Energetickou účinná řada","","","","A+++ ~ D","A+++ ~ D","","A+++ ~ D"]