{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":95,"n_cols":13,"rows_kept":95,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-R"]
[]
[]
[]
[]
["","","","","","ATXM20R2V1B §$ ATXM20R5V1B","ATXM20R2V1B","ATXM20R5V1B","ATXM25R2V1B","ATXM25R5V1B","ATXM35R2V1B","ATXM35R5V1B","ATXM50R2V1B"]
["Hladina akustického tlaku","Vytápění","","Vysoké","dBA","39"]
["","","","Střední","dBA","34"]
["","","","Tichý provoz","dBA","20"]
["","","","Nízký","dBA","26"]
["","Chlazení","","Střední","dBA","33"]
["","","","Tichý provoz","dBA","19"]
["","","","Nízký","dBA","25"]
["","","","Vysoké","dBA","41"]
["Standardní příslušenství","Příručka pro instalaci","","","","1"]
["","Manuální ovládání","","","","1"]
["","Bezdrátové dálkové ovládání","","","","1"]
["","Baterie AAA","","","","2"]
["","Držák dálkového ovládání","","","","1"]
["","Montážní deska","","","","1"]
["","Deodorizační filtr s apatitem titanu","","","","1"]
["","Upevňovací šrouby vnitřní jednotky","","","","2"]
["","Souprava adaptérů WLAN","","","","1"]
["Řídicí systémy","Wired remote control","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A67"]
["Spoje potrubí","Kapalina","","Vnější průměr","mm","6.35"]
["","Plyn","","Vnější průměr","mm","9.50"]
["","Vypouštění","","","","18"]
["Příkon","Chlazení","","Jm.","kW","0.029"]
["","Vytápění","","Jm.","kW","0.023"]
["Sound power level","Chlazení","","","dBA","58"]
["","Vytápění","","","dBA","55"]
["Rozměry","Jednotka","","Šířka","mm","778"]
["","","","Hloubka","mm","272"]
["","","","Výška","mm","295"]
["Opláštění","Barva","","","","Bílý"]
["Hmotnost","Jednotka","","","kg","10.0"]
["Ventilátor","Průtok vzduchu","Vytápění","Vysoké","m³/min","9.3"]
["","","","Střední","m³/min","8.2"]
["","","","Nízký","m³/min","6.2"]
["","","","Tichý provoz","m³/min","5.1"]
["","","Chlazení","Nízký","m³/min","5.7"]
["","","","Střední","m³/min","7.5"]
["","","","Vysoké","m³/min","10.5"]
["","","","Tichý provoz","m³/min","4.3"]
["Power supply","Fáze","","","","1~"]
["","Označení","","","","V1"]
["","Frekvence","","","Hz","50"]
["","Napětí","","","V","220-240"]
["Poznámky","","","","","(1) - Køling: indendørs temp: 27 °CDB, 19,0 °CWB; udendørs temp. 35°CDB, 24°CWB; tilsvarende rørlængde: 5m"]
["","","","","","(2) - Vytápění: vnitřní teplota 20° CDB; vnější teplota 7° CDB, 6° CWB ekvivalentní délka potrubí chladiva: 5m"]
["Vstup napájení","Chlazení","","Jm.","kW","","0.029","0.029","0.029","0.029","0.03","0.03","0.03"]
["","Vytápění","","Jm.","kW","","0.023","0.023","0.022","0.022","0.027","0.027","0.032"]
["Opláštění","Barva","","","","","Bílá","Bílá","Bílá","Bílá","Bílá","Bílá","Bílá"]
["Rozměry","Jednotka","","Výška","mm","","295","295","295","295","295","295","299"]
["","","","Šířka","mm","","778","778","778","778","778","778","998"]
["","","","Hloubka","mm","","272","272","272","272","272","272","292"]
["Hmotnost","Jednotka","","","kg","","10","10","10","10","10","10","14.5"]
["Ventilátor","Průtok vzduchu","Chlazení","Vysoké","m³/min","","10.5","10.5","10.5","10.5","11.3","11.3","15.8"]
["","","","Střední","m³/min","","7.5","7.5","7.6","7.6","7.8","7.8","14"]
["","","","Nízký","m³/min","","5.7","5.7","5.7","5.7","6","6","11.4"]
["","","","Tichý provoz","m³/min","","4.3","4.3","4.1","4.1","4.2","4.2","8.3"]
["","","Vytápění","Vysoké","m³/min","","9.3","9.3","9.8","9.8","9.8","9.8","15.8"]
["","","","Střední","m³/min","","8.2","8.2","8","8","8.5","8.5","14.2"]
["","","","Nízký","m³/min","","6.2","6.2","6.3","6.3","6.5","6.5","12"]
["","","","Tichý provoz","m³/min","","5.1","5.1","4.9","4.9","4.9","4.9","10.5"]
["Hladina akustického výkonu","Chlazení","","","dBA","","58","58","58","58","58","58","58"]
["","Vytápění","","","dBA","","55","55","55","55","55","55","58"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","","41","41","41","41","45","45","44"]
["","","","Střední","dBA","","33","33","33","33","33","33","40"]
["","","","Nízký","dBA","","25","25","25","25","25","25","36"]
["","","","Tichý provoz","dBA","","19","19","19","19","19","19","27"]
["","Vytápění","","Vysoké","dBA","","39","39","39","39","39","39","43"]
["","","","Střední","dBA","","34","34","34","34","35","35","39"]
["","","","Nízký","dBA","","26","26","27","27","28","28","34"]
["","","","Tichý provoz","dBA","","20","20","20","20","20","20","31"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Plyn","","Vnější průměr","mm","","9.5","9.5","9.5","9.5","9.5","9.5","12.7"]
["","Odvod kondenzátu","","","","","18","18","18","18","18","18","18"]
["Řídicí systémy","Infrared remote control","","","","","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67"]
["Řídicí systémy","Kabelové dálkové ovládání","","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standardní příslušenství","Installation manual","","","","","1","1","1","1","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","","2","2","2","2","2","2","2"]
["","WLAN adapter kit","","","","","1","1","1","1","1","1","1"]
["","Operation manual","","","","","1","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","1","1","1","1","1","1","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","1","1"]
["Napájení","Označení","","","","","V1","V1","V1","V1","V1","V1","V1"]
["","Fáze","","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Frekvence","","","Hz","","50","50","50","50","50","50","50"]
["","Napětí","","","V","","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standardní příslušenství","Silver particle filter","","","","","","","","","","","1"]