{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":7,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-N / ARXP-N"]
[]
[]
[]
[]
["","","","","ATXP20N5V1B / ARXP20N5V1B","ATXP25N5V1B / ARXP25N5V1B","ATXP35N5V1B / ARXP35N5V1B"]
["Venkovní jednotka","","","","ARXP20N5V1B","ARXP25N5V1B","ARXP35N5V1B"]
["Chladicí výkon","Min.","","kW","1.3","1.3","1.3"]
["","Jm.","","kW","2.00","2.50","3.50"]
["","Max.","","kW","2.6","3.0","4.0"]
["Topný výkon","Min.","","kW","1.30","1.30","1.30"]
["","Jm.","","kW","2.50","3.00","4.00"]
["","Max.","","kW","3.50","4.00","4.80"]
["Jmenovitá účinnost","COP","","","4.77","4.36","4.02"]
["","EER","","","3.71","3.71","3.24"]
["","Směrnice oenergetických štítcích","Chlazení","","A","A","A"]
["","","Vytápění","","A","A","A"]
["Poznámky","","","","(1) - Jmenovité chladicí výkony vycházejí z těchto podmínek: vnitřní teplota: 27°CDB, 19°CWB, venkovní teplota: 35 °CDB, ekvivalentní délka potrubí s chladivem: 5 m, rozdíl úrovní: 0 m.","(1) - Jmenovité chladicí výkony vycházejí z těchto podmínek: vnitřní teplota: 27°CDB, 19°CWB, venkovní teplota: 35 °CDB, ekvivalentní délka potrubí s chladivem: 5 m, rozdíl úrovní: 0 m.","(1) - Jmenovité chladicí výkony vycházejí z těchto podmínek: vnitřní teplota: 27°CDB, 19°CWB, venkovní teplota: 35 °CDB, ekvivalentní délka potrubí s chladivem: 5 m, rozdíl úrovní: 0 m."]
["","","","","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m.","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m.","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]
["","","","","(3) - Údaje o elektrickém systému najdete v samostatném výkresu","(3) - Údaje o elektrickém systému najdete v samostatném výkresu","(3) - Údaje o elektrickém systému najdete v samostatném výkresu"]