{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":7,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXTP-K"]
[]
[]
[]
[]
["","","","","","ATXTP25K3V1B","ATXTP35K3V1B"]
["Vstup napájení","Chlazení","","Jm.","kW","0.03","0.03"]
["","Vytápění","","Jm.","kW","0.035","0.035"]
["Opláštění","Barva","","","","Bílá","Bílá"]
["Rozměry","Jednotka","","Výška","mm","285","285"]
["","","","Šířka","mm","770","770"]
["","","","Hloubka","mm","225","225"]
["Hmotnost","Jednotka","","","kg","9","9"]
["Ventilátor","Průtok vzduchu","Chlazení","Vysoké","m³/min","10.6","11.4"]
["","","","Střední","m³/min","7.7","8.2"]
["","","","Nízký","m³/min","5.3","5.4"]
["","","","Tichý provoz","m³/min","4.3","4.3"]
["","","Vytápění","Vysoké","m³/min","11.2","10.8"]
["","","","Střední","m³/min","8","7.8"]
["","","","Nízký","m³/min","5.8","5.8"]
["","","","Tichý provoz","m³/min","4.9","4.9"]
["Hladina akustického výkonu","Chlazení","","","dBA","58","58"]
["","Vytápění","","","dBA","58","58"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","43","43"]
["","","","Střední","dBA","35","35"]
["","","","Nízký","dBA","26","26"]
["","","","Tichý provoz","dBA","21","21"]
["","Vytápění","","Vysoké","dBA","43","43"]
["","","","Střední","dBA","35","35"]
["","","","Nízký","dBA","26","26"]
["","","","Tichý provoz","dBA","21","21"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","6.35","6.35"]
["","Plyn","","Vnější průměr","mm","9.5","9.5"]
["","Odvod kondenzátu","","","","16 (vnitřní průměr připojované hadice)","16 (vnitřní průměr připojované hadice)"]
["Řídicí systémy","Infrared remote control","","","","ARC480A11","ARC480A11"]
["Řídicí systémy","Kabelové dálkové ovládání","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standardní příslušenství","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Napájení","Označení","","","","V1","V1"]
["","Fáze","","","","1~","1~"]
["","Frekvence","","","Hz","50","50"]
["","Napětí","","","V","220-240","220-240"]