{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":7,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BPMKS967A"]
[]
[]
[]
[]
["","","","","","BPMKS967B2B","BPMKS967B3B"]
["Standardní příslušenství","Příručka pro instalaci","","","","1","1"]
["","Reduktor pro vnější jednotku; průměr strany plynu 12.7","","","","1","1"]
["","Reduktor pro vnější jednotku; průměr strany plynu 15,9","","","","1","1"]
["","Reduktor pro vnější jednotku; průměr strany plynu 19,1","","","","1","1"]
["","Reduktor pro vnější jednotku; průměr strany kapaliny 6.4","","","","1","1"]
["","Reduktor pro vnitřní jednotku; průměr strany plynu 9.52","","","","1","1"]
["","Reduktor pro vnitřní jednotku; průměr strany kapaliny 12.7","","","","2","3"]
["","Reduktor pro vnitřní jednotku; průměr strany kapaliny 9,5","","","","2","3"]
["","Kovový závěs","","","","4","4"]
["","Šrouby (M4x8)","","","","8","8"]
["","Tepelná izolace","","","","3","4"]
["","Vázací páska","","","","2","2"]
["Rozměry","Jednotka","","Šířka","mm","650","650"]
["","","","Hloubka","mm","350","350"]
["","","","Výška","mm","180","180"]
["Hmotnost","Jednotka","","","kg","7.5","8"]
["Connectable indoor unit type","","","","","Třída 20 – třída 71","Třída 20 – třída 71"]
["Spoje potrubí","Venkovní jednotka","Kapalný","Piping connections-=-Outdoor unit-=-Liquid-=-Quantity","","1","1"]
["","","","Piping connections-=-Outdoor unit-=-Liquid-=-ID-=-mm","mm","9.5","9.5"]
["","","Plyn","Piping connections-=-Outdoor unit-=-Gas-=-Quantity-=-mm","mm","1","1"]
["","","","Piping connections-=-Outdoor unit-=-Gas-=-ID-=-mm","mm","19.1","19.1"]
["","Vnitřní jednotka","Plyn","Piping connections-=-Indoor unit-=-Gas-=-Quantity-=-mm","mm","2","3"]
["","","","Piping connections-=-Indoor unit-=-Gas-=-ID-=-mm","mm","15.9","15.9"]
["","","Kapalný","Piping connections-=-Indoor unit-=-Liquid-=-ID-=-mm","mm","6.4","6.4"]
["","","","Piping connections-=-Indoor unit-=-Liquid-=-Quantity","","2","3"]
["","Vypouštění","","ID","mm","Úprava vypouštěné kapaliny","Úprava vypouštěné kapaliny"]
["Příkon","Nom.","","","kW","0.010","0.010"]
["Power supply","Frekvence","","","Hz","50","50"]
["","Napětí","","","V","230","230"]