{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BR00000678"]
[]
[]
[]
[]
["","","","","","BR00000678."]
["Použití","","","","","Parapetní typ"]
["Výkon","m³/min","","","","33.33"]
["Opláštění","Barva","","","","Povrchová úprava v provedení lakované pozinkované oceli"]
["Rozměry","Jednotka","","Výška","mm","1628"]
["","","","Šířka","mm","720"]
["","","","Hloubka","mm","770"]
["Hmotnost","Jednotka","","","kg","150"]
["Využitelná plocha místnosti","m²","","","","133"]
["Operace čištění vzduchu","Vstup napájení","","H","kW","0.379"]
["Hladina akustického tlaku","Operace čištění vzduchu","","Vysoké","dBA","55.9"]
["Ventilátor","Průtok vzduchu","Operace čištění vzduchu","Turbo","m³/h","2300"]
["","","","Vysoké","m³/h","2000"]
["Bezpečnostní zařízení","Položka","","01","","Bezpečnostní spínač (zastavení provozu při otevření zadního panelu)"]
["Standardní příslušenství","Prefilter selected","","","","1"]
["","HEPA filter selected","","","","1"]
["","Quick Start and Maintenance Guide","","","","1"]
["","Installation and Operation Manual available for download","","","","1"]
["Napájecí šňůra","m","","","","3"]
["Napájení","Frekvence","","","Hz","50/60"]
["Proud při provozu","Operace čištění vzduchu","","Vysoké","A","1.73"]