{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1E53A"]
[]
[]
[]
[]
["","","","","BRC1E53A7"]
["Opláštění","Barva","","","Čerstvý bílý"]
["","Kryt tlačítka","","","Ne"]
["","Provozní LED","Barva","","Zelená"]
["Rozměry","Jednotka","Výška","mm","120"]
["","","Šířka","mm","120"]
["","","Hloubka","mm","19"]
["","Jednotka v obalu","Výška","mm","55"]
["","","Šířka","mm","160"]
["","","Hloubka","mm","150"]
["Hmotnost","Jednotka","","kg","0.200"]
["","Jednotka v obalu","","kg","0.415"]
["Balení","Materiál","","","Kartón_"]
["","Hmotnost","","kg","0.05"]
["LCD","Typ","","","Full dot (160 x 255)"]
["","Rozměry","Výška","mm","43.2"]
["","","Šířka","mm","68.85"]
["","Zadní světlo","Barva","","Bílý"]
["Teplota okolí","Režim","Min.","°C","-10"]
["","","Max.","°C","50"]
["","Skladování","Min.","°C","-20"]
["","","Max.","°C","70"]
["","Relativní vlhkost <","","%","95"]
["Kabelové spoje","Délka kabeláže","Max.","m","500"]
["Záloha pro výpadek napájení","","","","Ano (hodiny budou funkční po dobu nepřekračující 48 hodin)"]