{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1HHDW"]
[]
[]
[]
[]
["","","","","BRC1HHDAW (Archived)"]
["Opláštění","Barva","","","Bílá"]
["Skříň","Kryt tlačítka","","","Ne"]
["","Provozní LED","Barva","","Modrý stavový indikátor"]
["Rozměry","Jednotka","Výška","mm","85"]
["","","Šířka","mm","85"]
["","","Hloubka","mm","25"]
["","Jednotka v obalu","Výška","mm","50"]
["","","Šířka","mm","217"]
["","","Hloubka","mm","161"]
["Hmotnost","Jednotka","","kg","0.110"]
["","Jednotka v obalu","","kg","0.317"]
["Balení","Materiál","","","Karton"]
["","Hmotnost","","kg","0.0850"]
["LCD","Typ","","","100 x 150 bodů"]
["","Rozměry","Výška","mm","40.7"]
["","","Šířka","mm","28.0"]
["","Zadní světlo","Barva","","Bílá"]
["Teplota prostředí","Režim","Min.","°C","-10"]
["","","Max.","°C","52"]
["","Skladování","Min.","°C","-20"]
["","","Max.","°C","70"]
["","Teplota prostředí-=-Relativní vlhkost <-=-%","","%","95"]
["Řídicí systémy","Třída řízení teploty","","","VI"]
["","Přínos k celoroční účinnosti prostorového vytápění","","%","4.0"]
["Kabelové spoje","Délka kabeláže","Max.","m","500"]