{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":8,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHYHBH-AV32"]
[]
[]
[]
[]
["","","","","","CHYHBH05AAV32","CHYHBH05AFV32","CHYHBH08AFV32"]
["Opláštění","Barva","","","","Bílá","Bílá","Bílá"]
["","Materiál","","","","Povrstvený plech","Povrstvený plech","Povrstvený plech"]
["Rozměry","Jednotka","","Výška","mm","902","902","902"]
["","","","Šířka","mm","450","450","450"]
["","","","Hloubka","mm","164","164","164"]
["Hmotnost","Jednotka","","","kg","30.0","30.0","30.0"]
["PED","Kategorie","","","","","Čl.3§3, Vyjmuto z rozsahu PED kvůli čl. 1, pol. 3.6 z 97/23/ES","Čl.3§3, Vyjmuto z rozsahu PED kvůli čl. 1, pol. 3.6 z 97/23/ES"]
["Vodní strana Výměník tepla","Průtok vody","Vytápění","Max.","l/min","23.0 (5)","23.0 (5)","23.0 (5)"]
["Hladina akustického výkonu","Jm.","","","dBA","42 (6)","42 (6)","42 (6)"]
["Provozní rozsah","Vytápění","Vody strana","Min.","°C","25 (7)","25 (7)","25 (7)"]
["","","","Max.","°C","50 (7)","50 (7)","50 (7)"]
["Napájení","Označení","","","","V3","V3","V3"]
["","Fáze","","","","1~","1~","1~"]
["","Frekvence","","","Hz","50","50","50"]
["","Napětí","","","V","230","230","230"]
["Kabelové spoje","Kabelové spoje-=-Pro spojení s&nbsp;uživatelským rozhraním","","Kabelové spoje-=-Pro spojení s&nbsp;uživatelským rozhraním-=-Množství","","2","2","2"]
["Kabelov é spoje","Pro spojení s uživatelsk ým rozhraním","","Poznámka","","0,75 mm² až 1,25 mm² (max délka 500 m)","0,75 mm² až 1,25 mm² (max délka 500 m)","0,75 mm² až 1,25 mm² (max délka 500 m)"]
["Poznámky","","","","","(1) - Pouze pro vnitřní jednotku","(1) - Pouze pro vnitřní jednotku","(1) - Pouze pro vnitřní jednotku"]
["","","","","","(2) - ST/MT 7°C/6°C - LWC 35°C (DT=5°C), obtok kotle","(2) - ST/MT 7°C/6°C - LWC 35°C (DT=5°C), obtok kotle","(2) - ST/MT 7°C/6°C - LWC 35°C (DT=5°C), obtok kotle"]
["","","","","","(3) - ST/MT 7°C/6°C - LWC 45°C (DT=5°C), obtok kotle","(3) - ST/MT 7°C/6°C - LWC 45°C (DT=5°C), obtok kotle","(3) - ST/MT 7°C/6°C - LWC 45°C (DT=5°C), obtok kotle"]
["","","","","","(4) - Min. required","(4) - Min. required","(4) - Min. required"]
["","","","","","(5) - Obtok kotle","(5) - Obtok kotle","(5) - Obtok kotle"]
["","","","","","(6) - Podle EN14825","(6) - Podle EN14825","(6) - Podle EN14825"]
["","","","","","(7) - Informace o provozním rozsahu *HYHB* a *HYKOMB33AA naleznete v příslušném výkrese","(7) - Informace o provozním rozsahu *HYHB* a *HYKOMB33AA naleznete v příslušném výkrese","(7) - Informace o provozním rozsahu *HYHB* a *HYKOMB33AA naleznete v příslušném výkrese"]