{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-BS"]
[]
[]
[]
[]
["","","","","","CTXA15B2V1BS"]
["Vstup napájení","Chlazení","","Jm.","kW","0.02"]
["","Vytápění","","Jm.","kW","0.02"]
["Opláštění","Barva","","","","Stříbrný"]
["Rozměry","Jednotka","","Výška","mm","295"]
["","","","Šířka","mm","798"]
["","","","Hloubka","mm","189"]
["Hmotnost","Jednotka","","","kg","11.5"]
["Ventilátor","Průtok vzduchu","Chlazení","Vysoké","m³/min","11"]
["","","","Střední","m³/min","8.2"]
["","","","Nízký","m³/min","6.1"]
["","","","Tichý provoz","m³/min","4.6"]
["","","Vytápění","Vysoké","m³/min","10.9"]
["","","","Střední","m³/min","8.7"]
["","","","Nízký","m³/min","6.4"]
["","","","Tichý provoz","m³/min","4.5"]
["Hladina akustického výkonu","Chlazení","","","dBA","57"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","39"]
["","","","Střední","dBA","32"]
["","","","Nízký","dBA","25"]
["","","","Tichý provoz","dBA","21"]
["","Vytápění","","Vysoké","dBA","39"]
["","","","Střední","dBA","32"]
["","","","Nízký","dBA","25"]
["","","","Tichý provoz","dBA","21"]
["Chladivo","Vliv na globální oteplování (GWP)","","","","675"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","6.35"]
["","Plyn","","Vnější průměr","mm","9.5"]
["","Odvod kondenzátu","","","","18"]
["Řídicí systémy","Infračervené dálkové ovládání","","","","ARC466A58"]
["","Kabelové dálkové ovládání","","","","BRC073"]
["Standardní příslušenství","Installation manual","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Air filter","","","","2"]
["","Infrared remote control","","","","1"]
["","Remote controller mounting plate","","","","1"]
["","Screw bag","","","","1"]
["Napájení","Označení","","","","V1"]
["","Fáze","","","","1~"]
["","Frekvence","","","Hz","50"]
["","Napětí","","","V","220-240"]