{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":9,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXS-K"]
[]
[]
[]
[]
["","","","","","CTXS15K2V1B","CTXS15K3V1B","CTXS35K2V1B","CTXS35K3V1B"]
["Hladina akustického tlaku","Vytápění","","Vysoké","dBA","38","","41"]
["","","","Tichý provoz","dBA","21","","21"]
["","","","Nízký","dBA","28","","30"]
["","Chlazení","","Tichý provoz","dBA","21","","21"]
["","","","Nízký","dBA","25","","28"]
["","","","Vysoké","dBA","37","","42"]
["","","","Jm.","dBA","33"]
["","Chlazení","","Jm.","dBA","31","","35"]
["Standardní příslušenství","Příručka pro instalaci","","","","1","","1"]
["","Manuální ovládání","","","","1","","1"]
["","Bezdrátové dálkové ovládání","","","","1","","1"]
["","Baterie","","","","2","","2"]
["","Držák dálkového ovládání","","","","1","","1"]
["","Montážní deska","","","","1","","1"]
["","Upevňovací šrouby vnitřní jednotky","","","","2","","2"]
["","Fotokatalytický filtr s apatitem titanu pro čištění vzduchu","","","","2","","2"]
["Řídicí systémy","Infrared remote control","","","","ARC466A6","","ARC466A6"]
["Piping connections","Kapalina","","Vnější průměr","mm","6.35","","6.35"]
["","Plyn","","Vnější průměr","mm","9.5","","9.5"]
["","Vypouštění","","","","18","","18"]
["Příkon","Chlazení","","Jm.","kW","0.040","","0.040"]
["","Vytápění","","Jm.","kW","0.040","","0.040"]
["Hladina akustického výkonu","Chlazení","","","dBA","55","","59"]
["","Vytápění","","","dBA","56","","58"]
["Rozměry","Jednotka","","Šířka","mm","780","","780"]
["","","","Hloubka","mm","215","","215"]
["","","","Výška","mm","289","","289"]
["Opláštění","Colour","","","","Bílý","","Bílý"]
["Hmotnost","Jednotka","","","kg","8","","8"]
["Ventilátor","Průtok vzduchu","Vytápění","Vysoké","m³/min","","","10.1"]
["","","","Nízký","m³/min","","","6.3"]
["","","","Tichý provoz","m³/min","","","4.3"]
["","","Chlazení","Nízký","m³/min","","","5.2"]
["","","","Vysoké","m³/min","","","9.2"]
["","","","Tichý provoz","m³/min","","","3.9"]
["","","","Jm.","m³/min","","","8.1"]
["","","Chlazení","Jm.","m³/min","","","7.2"]
["Power supply","Phase","","","","1~","","1~"]
["","Frekvence","","","Hz","50","","50"]
["","Označení","","","","V1","","V1"]
["","Napětí","","","V","220-240","","220-240"]
["Poznámky","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["Vstup napájení","Chlazení","","Jm.","kW","","0.04","","0.040"]
["","Vytápění","","Jm.","kW","","0.04","","0.040"]
["Opláštění","Barva","","","","","Bílá","","Bílá"]
["Rozměry","Jednotka","","Výška","mm","","289","","289"]
["","","","Šířka","mm","","780","","780"]
["","","","Hloubka","mm","","215","","215"]
["Hmotnost","Jednotka","","","kg","","8","","8.00"]
["Ventilátor","Průtok vzduchu","Chlazení","Vysoké","m³/min","","7.9","","9.2"]
["","","","Střední","m³/min","","6.3","","7.2"]
["","","","Nízký","m³/min","","4.7","","5.2"]
["","","","Tichý provoz","m³/min","","3.9","","3.9"]
["","","Vytápění","Vysoké","m³/min","","9","","10.1"]
["","","","Střední","m³/min","","7.5","","8.1"]
["","","","Nízký","m³/min","","6","","6.3"]
["","","","Tichý provoz","m³/min","","4.3","","4.3"]
["Hladina akustického výkonu","Chlazení","","","dBA","","55","","59"]
["","Vytápění","","","dBA","","56","","58"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","","37","","42"]
["","","","Střední","dBA","","31","","35"]
["","","","Nízký","dBA","","25","","28"]
["","","","Tichý provoz","dBA","","21","","21"]
["","Vytápění","","Vysoké","dBA","","38","","41"]
["","","","Střední","dBA","","33","","36"]
["","","","Nízký","dBA","","28","","30"]
["","","","Tichý provoz","dBA","","21","","21"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","","6.35","","6.35"]
["","Plyn","","Vnější průměr","mm","","9.5","","9.50"]
["","Odvod kondenzátu","","","","","18","","18"]
["Řídicí systémy","Infrared remote control","","","","","ARC466A6","","ARC466A6"]
["Standardní příslušenství","Installation manual","","","","","1","","1"]
["","Wireless remote control","","","","","1","","1"]
["","AAA dry-cell batteries","","","","","2","","2"]
["","Operation manual","","","","","1","","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2"]
["","Indoor unit fixing screws","","","","","2","","2"]
["","Mounting plate","","","","","1","","1"]
["","Remote control holder","","","","","1","","1"]
["Napájení","Označení","","","","","V1","","V1"]
["","Fáze","","","","","1~","","1~"]
["","Frekvence","","","Hz","","50","","50"]
["","Napětí","","","V","","220-240","","220-240"]