{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CVXM-A9"]
[]
[]
[]
[]
["","","","","","CVXM20A3V1B9"]
["Vstup napájení","Chlazení","","Jm.","kW","0.02"]
["","Vytápění","","Jm.","kW","0.02"]
["Opláštění","Barva","","","","Bílá"]
["Rozměry","Jednotka","","Výška","mm","600"]
["","","","Šířka","mm","750"]
["","","","Hloubka","mm","238"]
["Hmotnost","Jednotka","","","kg","17"]
["Ventilátor","Průtok vzduchu","Chlazení","Vysoké","m³/min","8.7"]
["","","","Střední","m³/min","7"]
["","","","Nízký","m³/min","4.9"]
["","","","Tichý provoz","m³/min","4.1"]
["","","Vytápění","Vysoké","m³/min","9.2"]
["","","","Střední","m³/min","7.2"]
["","","","Nízký","m³/min","5.6"]
["","","","Tichý provoz","m³/min","4.1"]
["Hladina akustického výkonu","Chlazení","","","dBA","52"]
["","Vytápění","","","dBA","52"]
["Hladina akustického tlaku","Chlazení","","Vysoké","dBA","38"]
["","","","Střední","dBA","32"]
["","","","Nízký","dBA","25"]
["","","","Tichý provoz","dBA","22"]
["","Vytápění","","Vysoké","dBA","38"]
["","","","Střední","dBA","32"]
["","","","Nízký","dBA","25"]
["","","","Tichý provoz","dBA","21"]
["Chladivo","Vliv na globální oteplování (GWP)","","","","675"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","6.4"]
["","Plyn","","Vnější průměr","mm","9.5"]
["","Odvod kondenzátu","","","","VP20 (I.D. 20/O.D. 26)"]
["Control systems","Infrared remote control","","","","ARC466A66"]
["Řídicí systémy","Kabelové dálkové ovládání","","","","BRC073A1"]
["Standardní příslušenství","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Napájení","Fáze","","","","1~"]
["","Frekvence","","","Hz","50"]
["","Napětí","","","V","220-240"]