{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCC601A51"]
[]
[]
[]
[]
["","","","","","DCC601A51."]
["Příkon","kW","","","","0.015"]
["Max. počet připojitelných vnitřních jednotek:","","","","","32"]
["Max. počet připojitelných vnějších jednotek @","","","","","7"]
["Rozměry","Jednotka","","Výška","mm","136"]
["","","","Šířka","mm","384"]
["","","","Hloubka","mm","92"]
["Komunikace","DIII-NET","","Množství","","1"]
["","","","Poznámka","","DIII-NET (F1F2)"]
["","Ethernet","","Množství","","1"]
["","Vstupní terminál","Digitální","Množství","","4"]
["Teplota prostředí","Režim","","Min.","°C","-10"]
["","","","Max.","°C","50"]
["","Skladování","","Min.","°C","-20"]
["","","","Max.","°C","60"]
["","Teplota prostředí-=-Relativní vlhkost <-=-%","","","%","85"]
["Napájení","Frekvence","","","Hz","50/60"]
["","Napětí","","","V","110-240 AC"]
["Poznámky","","","","","(1) - Zahrnuje příkon napájecího zdroje WAGO, modul CPU a modul vstupu/výstupu"]
["","","","","","(2) - Rozměry zahrnují napájecí zdroj WAGO, modul CPU, modul vstupu/výstupu a potřebný prostor mezi jednotlivými součástmi"]
["","","","","","(3) - Rozměry doplňkové obrazovky jsou: výška: 209 mm, šířka: 123 mm, hloubka: 8,5 mm"]