{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCM601A51"]
[]
[]
[]
[]
["","","","","DCM601A51."]
["Teplota prostředí","Relativní vlhkost <","","%","85"]
["Max. počet připojitelných vnitřních jednotek:","","","","64, 512 (1), 2,560 (2)"]
["Příkon","kW","","","0.023"]
["Komunikace","DIII-NET","Množství","","1"]
["","Ethernet","Poznámka","","Přístup na internet (100BASE-TX)"]
["","","Množství","","1"]
["","Modem","Poznámka","","Monitorovací síťový servisní systém klimatizace"]
["Instalace","","","","Pouze svislý směr"]
["Rozměry","Jednotka","Šířka","mm","290"]
["","","Hloubka","mm","50"]
["","","Výška","mm","243"]
["Hmotnost","Jednotka","","kg","2.4"]
["Power supply","Frekvence","","Hz","50/60"]
["","Napětí","","V","AC 100-240"]
["Poznámky","","","","(1) - S 7 ITM a adaptéry"]
["","","","","(2) - S 5 ITM kombinované s ITM integrátorerm"]