{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":8,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EABH-D9W7 / EPGA011-016DV7"]
[]
[]
[]
[]
["","","","","","EABH16DF9W7 / EPGA11DAV37","EABH16DF9W7 / EPGA14DAV37","EABH16DF9W7 / EPGA16DAV37"]
["COP","","","","","5.15 (1), 3.88 (2)","4.99 (1), 3.65 (2)","4.78 (1), 3.71 (2)"]
["Indoor unit","","","","","EABH16DA9W7","EABH16DA9W7","EABH16DA9W7"]
["Prostorové vytápění","Výstup vody 55 °C v průměrném podnebí","Obecně","Třída celoroční účinnosti prostorového vytápění","","A++","A++","A++"]
["","","","ηs (Celoroční účinnost prostorového vytápění)","%","129","130","133"]
["","","","SCOP","","3.29","3.34","3.41"]
["Topný výkon","Jm.","","","kW","11.1 (1), 11.3 (2)","14.5 (1), 14.5 (2)","16.5 (1), 15.6 (2)"]
["Vstup napájení","Vytápění","","Jm.","kW","2.16 (1), 2.91 (2)","2.91 (1), 3.96 (2)","3.45 (1), 4.21 (2)"]
["Poznámky","","","","","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - Podmínky 2: chlazení Ta 35°C - LWE 7℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Podmínky 2: chlazení Ta 35°C - LWE 7℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Podmínky 2: chlazení Ta 35°C - LWE 7℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)"]