{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":9,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBSH-D"]
[]
[]
[]
[]
["","","","","","EBSH11P30DF","EBSH11P50DF","EBSH16P30DF","EBSH16P50DF"]
["Opláštění","Barva","","","","Dopravní bílá (RAL9016) / Dopravní černá (RAL9017)","Dopravní bílá (RAL9016) / Dopravní černá (RAL9017)","Dopravní bílá (RAL9016) / Dopravní černá (RAL9017)","Dopravní bílá (RAL9016) / Dopravní černá (RAL9017)"]
["","Materiál","","","","Polypropylén odolný proti nárazu","Polypropylén odolný proti nárazu","Polypropylén odolný proti nárazu","Polypropylén odolný proti nárazu"]
["Rozměry","Jednotka","","Výška","mm","1,893","1,910","1,893","1,910"]
["","","","Šířka","mm","594","792","594","792"]
["","","","Hloubka","mm","680","817","680","817"]
["Hmotnost","Jednotka","","","kg","93","114","93","114"]
["PED","Kategorie","","","","Kategorie II","Kategorie II","Kategorie II","Kategorie II"]
["Chladivo","Typ","","","","R-32","R-32","R-32","R-32"]
["","Vliv na globální oteplování (GWP)","","","","675.0","675.0","675.0","675.0"]
["","Náplň","","","kg","3.80","3.80","3.80","3.80"]
["","Náplň","","","tCO2Eq","2.57","2.57","2.57","2.57"]
["Hladina akustického výkonu","Jm.","","","dBA","44.7","44.7","49.0","49.0"]
["Hladina akustického tlaku","Jm.","","","dBA","36.8","36.8","40.3","40.3"]
["Provozní rozsah","Vytápění","Vody strana","Min.","°C","0","0","0","0"]
["","","","Max.","°C","0","0","0","0"]
["","Chlazení","Okolí","Min.","°CST","0","0","0","0"]
["","","Vody strana","Min.","°C","0","0","0","0"]
["","","","Max.","°C","0","0","0","0"]
["Napájení","Fáze","","","","1~","1~","1~","1~"]
["","Frekvence","","","Hz","50","50","50","50"]
["","Napětí","","","V","230","230","230","230"]
["Poznámky","","","","","(1) - Tepelná ztráta podle EN12897","(1) - Tepelná ztráta podle EN12897","(1) - Tepelná ztráta podle EN12897","(1) - Tepelná ztráta podle EN12897"]
["","","","","","(2) - Provozní limity viz výkres","(2) - Provozní limity viz výkres","(2) - Provozní limity viz výkres","(2) - Provozní limity viz výkres"]