{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSAX-D9W"]
[]
[]
[]
[]
["","","","","","EGSAX06DA9W","EGSAX10DA9W"]
["Topný výkon","Min.","","","kW","0.85","0.85"]
["","Jm.","","","kW","3.35","5.49"]
["","Max.","","","kW","7.98","9.55"]
["Vstup napájení","Nom.","","","kW","0.74","1.17"]
["COP","","","","","4.51","4.70"]
["Opláštění","Barva","","","","Bílá + černá","Bílá + černá"]
["","Materiál","","","","Povrstvený plech"]
["Rozměry","Jednotka","","Výška","mm","1,891","1,891"]
["","","","Šířka","mm","597","597"]
["","","","Hloubka","mm","666","666"]
["Hmotnost","Jednotka","","","kg","222","222"]
["Nádrž","Objem vody","","","l","180"]
["","Izolace","","Tepelná ztráta","kWh/24 h","1.2","1.2"]
["","Ochrana proti korozi","","","","Moření","Moření"]
["Chladivo","Typ","","","","R-32","R-32"]
["","Vliv na globální oteplování (GWP)","","","","675.0","675.0"]
["","Náplň","","","kg","1.70","1.70"]
["Provozní rozsah","Operation range-=-Installation space","","Operation range-=-Installation space-=-Min.-=-°C","°C","5","5"]
["","","","Operation range-=-Installation space-=-Max.-=-°C","°C","35","35"]
["","Operation range-=-Brine side","","Operation range-=-Brine side-=-Min.-=-°C","°C","-10","-10"]
["","","","Operation range-=-Brine side-=-Max.-=-°C","°C","30","30"]
["","Vytápění","Vody strana","Min.","°C","5","5"]
["","","","Max.","°C","65","65"]
["","Teplá užitková voda","Vody strana","Min.","°C","25","25"]
["","","","Max.","°C","60","60"]
["Prostorové vytápění","Výstup vody 55 °C v průměrném podnebí","Obecně","SCOP","","3.77 (1)","4.05 (1)"]
["","","","Třída celoroční účinnosti prostorového vytápění","","A++","A+++"]
["","Výstup vody 35°C vprůměrném podnebí","Obecné","SCOP","","5.18 (1)","5.20 (1)"]
["","","","Třída celoroční účinnosti prostorového vytápění","","A+++","A+++"]
["Power supply","Fáze","","","","1~/3~","1~/3~"]
["","Frekvence","","","Hz","50","50"]
["","Napětí","","","V","230/400","230/400"]
["Proud","Doporučené jištění","","","A","16/32","16/32"]
["Poznámky","","","","","(1) - Podle norem EN14825 a EN14511:2018","(1) - Podle norem EN14825 a EN14511:2018"]
["","","","","","(2) - Viz výkres s provozním rozsahem: zvýšení rozsahu podpůrným pomocným ohřívačem nebo záložním ohřívačem","(2) - Viz výkres s provozním rozsahem: zvýšení rozsahu podpůrným pomocným ohřívačem nebo záložním ohřívačem"]