{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSQH-A9W"]
[]
[]
[]
[]
["","","","","","EGSQH10S18AA9W"]
["Hladina akustického tlaku","Jm.","","","dBA","32.0 (6)"]
["Chladivo","Vliv na globální oteplování (GWP)","","","","2,090"]
["","Náplň","","","kg","1.80"]
["","Typ","","","","R-410A"]
["Provozní rozsah","Prostor pro instalaci","","Min.","°C","5.00"]
["","","","Max.","°C","30.0"]
["","Vytápění","Vody strana","Max.","°C","60.0 (7), 65.0 (8)"]
["","","","Min.","°C","24 (7), 24 (8)"]
["","Strana solanky","","Min.","°C","-5.00"]
["","","","Max.","°C","20.0"]
["","Teplá užitková voda","Vody strana","Max.","°C","55 (7), 60 (9)"]
["","","","Min.","°C","25 (7), 25 (9)"]
["Vstup napájení","Nom.","","","kW","2.38 (1), 2.89 (2)"]
["Hladina akustického výkonu","Nom.","","","dBA","46.0"]
["COP","","","","","4.33 (1), 3.18 (2)"]
["Rozměry","Jednotka","","Šířka","mm","600"]
["","","","Hloubka","mm","728"]
["","","","Výška","mm","1,730"]
["Opláštění","Materiál","","","","Povrstvený plech"]
["","Colour","","","","Bílý"]
["Zásobník","Objem vody","","","l","180"]
["","Ochrana proti korozi","","","","Anoda"]
["","Izolace","","Tepelná ztráta","kWh/24 h","1.36 (4)"]
["Hmotnost","Jednotka","","","kg","210"]
["Prostorové vytápění","Výstup vody 35°C v průměrném podnebí","Obecné","ηs (Celoroční účinnost prostorového vytápění)","%","194"]
["","","","Třída celoroční účinnosti prostorového vytápění","","A+++"]
["","","","SCOP","","5.06"]
["","Výstup vody 55 °C v průměrném podnebí","Obecně","Třída celoroční účinnosti prostorového vytápění","","A++"]
["","","","ηs (Celoroční účinnost prostorového vytápění)","%","139"]
["","","","SCOP","","3.68"]
["Topný výkon","Jm.","","","kW","10.3 (1), 9.20 (2)"]
["","Min.","","","kW","3.11 (1), 2.47 (2)"]
["","Max.","","","kW","13.0 (1), 11.9 (2)"]
["Power supply","Phase","","","","3~"]
["","Označení","","","","9W"]
["","Frekvence","","","Hz","50"]
["","Napětí","","","V","400"]
["Proud","Doporučené jištění","","","A","25"]
["Poznámky","","","","","(1) - EWB/LWB 0°C/-3°C - LWC 35°C (DT=5°C)"]
["","","","","","(2) - EWB/LWB 0°C/-3°C - LWC 45°C (DT=5°C)"]
["","","","","","(3) - s 40 % propylen glykolu"]
["","","","","","(4) - Tepelná ztráta podle EN12897"]
["","","","","","(5) - med rørføring + PHE + ekstra sikkerhedsvarmer; uden ekspansionskar"]
["","","","","","(6) - Hladina akustického tlaku je měřena pomocí mikrofonu umístěného ve vzdálenosti 1 m od jednotky. Jedná se o relativní hodnotu, která závisí na vzdálenosti a akustickém prostředí"]
["","","","","","(7) - U tepelného čerpadla"]
["","","","","","(8) - U tepleného čerpadla + záložního vytápění"]
["","","","","","(9) - U záložního vytápění"]