{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":11,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHBH-E6V / ERGA04-08EVA"]
[]
[]
[]
[]
["","","","","","EHBH04EA6V / ERGA04EAV3A","EHBH04EF6V / ERGA04EAV3A","EHBH08EA6V / ERGA06EAV3A","EHBH08EF6V / ERGA06EAV3A","EHBH08EA6V / ERGA08EAV3A","EHBH08EF6V / ERGA08EAV3A"]
["Topný výkon","Jm.","","","kW","4.30 (1), 4.60 (2)","4.30 (1), 4.60 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)"]
["Vstup napájení","Vytápění","","Jm.","kW","0.850 (1), 1.26 (2)","0.850 (1), 1.26 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)"]
["COP","","","","","5.10 (1), 3.65 (2)","5.10 (1), 3.65 (2)","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)"]
["Prostorové vytápění","Prostorové vytápění-=-Výstup vody 55&nbsp;°C v&nbsp;průměrném podnebí","Prostorové vytápění-=-Výstup vody 55&nbsp;°C v&nbsp;průměrném podnebí-=-Obecné","Prostorové vytápění-=-Výstup vody 55&nbsp;°C v&nbsp;průměrném podnebí-=-Obecné-=-SCOP","","3.26","3.26","3.25","3.25","3.27","3.27"]
["","","Prostorové vytápění-=-Výstup vody 55&nbsp;°C v&nbsp;průměrném podnebí-=-Obecně","Prostorové vytápění-=-Výstup vody 55&nbsp;°C v&nbsp;průměrném podnebí-=-Obecně-=-Třída celoroční účinnosti prostorového vytápění","","A++","A++","A++","A++","A++","A++"]
["","Prostorové vytápění-=-Výstup vody 35°C v&nbsp;průměrném podnebí","Prostorové vytápění-=-Výstup vody 35°C v&nbsp;průměrném podnebí-=-Obecné","Prostorové vytápění-=-Výstup vody 35°C v&nbsp;průměrném podnebí-=-Obecné-=-SCOP","","4.48","4.48","4.47","4.47","4.56","4.56"]
["","","","Prostorové vytápění-=-Výstup vody 35°C v&nbsp;průměrném podnebí-=-Obecné-=-Třída celoroční účinnosti prostorového vytápění","","A+++","A+++","A+++","A+++","A+++","A+++"]
["Poznámky","","","","","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - Podmínky 2: chlazení Ta 35°C - LWE 7℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Podmínky 2: chlazení Ta 35°C - LWE 7℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Podmínky 2: chlazení Ta 35°C - LWE 7℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Podmínky 2: chlazení Ta 35°C - LWE 7℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Podmínky 2: chlazení Ta 35°C - LWE 7℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Podmínky 2: chlazení Ta 35°C - LWE 7℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)"]