{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":13,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSX-E"]
[]
[]
[]
[]
["","","","","","EHSX04P30EF","EHSX04P50EF","EHSX04P50EG","EHSX04P30EG","EHSX08P30EF","EHSX08P50EF","EHSX08P50EG","EHSX08P30EG"]
["Opláštění","Barva","","","","Dopravní bílá (RAL9016) / Dopravní černá (RAL9017)","Dopravní bílá (RAL9016) / Dopravní černá (RAL9017)","Dopravní bílá (RAL9016) / Dopravní černá (RAL9017)","Dopravní bílá (RAL9016) / Dopravní černá (RAL9017)","Dopravní bílá (RAL9016) / Dopravní černá (RAL9017)","Dopravní bílá (RAL9016) / Dopravní černá (RAL9017)","Dopravní bílá (RAL9016) / Dopravní černá (RAL9017)","Dopravní bílá (RAL9016) / Dopravní černá (RAL9017)"]
["","Materiál","","","","Polypropylén odolný proti nárazu","Polypropylén odolný proti nárazu","Polypropylén odolný proti nárazu","Polypropylén odolný proti nárazu","Polypropylén odolný proti nárazu","Polypropylén odolný proti nárazu","Polypropylén odolný proti nárazu","Polypropylén odolný proti nárazu"]
["Rozměry","Jednotka","","Výška","mm","1,892","1,905","1,910","1,891","1,892","1,905","1,910","1,891"]
["","","","Šířka","mm","594","792","792","594","594","792","792","594"]
["","","","Hloubka","mm","644","812","817","644","644","812","817","644"]
["Hmotnost","Jednotka","","","kg","77","107","97.0","77.0","77","107","97.0","77.0"]
["PED","Kategorie","","","","Čl. 4.3","Čl. 4.3","Čl. 4.3","Čl. 4.3","Čl. 4.3","Čl. 4.3","Čl. 4.3","Čl. 4.3"]
["Chladivo","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Vliv na globální oteplování (GWP)","","","","675","675","675.0","675.0","675","675","675.0","675.0"]
["","Náplň","","","kg","1.5","1.5","1.50","1.50","1.5","1.5","1.50","1.50"]
["Hladina akustického výkonu","Jm.","","","dBA","39","39","39","39","39","39","39","39"]
["Provozní rozsah","Vytápění","Vody strana","Min.","°C","18","18","18","18","18","18","18","18"]
["","","","Max.","°C","65","65","65","65","65","65","65","65"]
["","Chlazení","Okolí","Min.","°CST","10","10","10","10","10","10","10","10"]
["","","Vody strana","Min.","°C","5","5","5","5","5","5","5","5"]
["","","","Max.","°C","22","22","22","22","22","22","22","22"]
["Napájení","Fáze","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frekvence","","","Hz","50","50","50","50","50","50","50","50"]
["","Napětí","","","V","230","230","230","230","230","230","230","230"]
["Poznámky","","","","","(1) - Tepelná ztráta podle EN12897","(1) - Tepelná ztráta podle EN12897","(1) - Tepelná ztráta podle EN12897","(1) - Tepelná ztráta podle EN12897","(1) - Tepelná ztráta podle EN12897","(1) - Tepelná ztráta podle EN12897","(1) - Tepelná ztráta podle EN12897","(1) - Tepelná ztráta podle EN12897"]