{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":9,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSXB-D3"]
[]
[]
[]
[]
["","","","","","EHSXB04P30DA3","EHSXB04P50DA3","EHSXB08P30DA3","EHSXB08P50DA3"]
["Opláštění","Barva","","","","Dopravní bílá (RAL9016) / Tmavě šedá (RAL7011)","Dopravní bílá (RAL9016) / Tmavě šedá (RAL7011)","Dopravní bílá (RAL9016) / Tmavě šedá (RAL7011)","Dopravní bílá (RAL9016) / Tmavě šedá (RAL7011)"]
["","Materiál","","","","Polypropylén odolný proti nárazu","Polypropylén odolný proti nárazu","Polypropylén odolný proti nárazu","Polypropylén odolný proti nárazu"]
["Rozměry","Jednotka","","Výška","mm","1891","1896","1891","1896"]
["","","","Šířka","mm","595","790","595","790"]
["","","","Hloubka","mm","615","790","615","790"]
["Hmotnost","Jednotka","","","kg","76.0","99.0","76.0","99.0"]
["PED","Kategorie","","","","čl. 3.3","čl. 3.3","čl. 3.3","čl. 3.3"]
["Chladivo","Typ","","","","R-32","R-32","R-32","R-32"]
["","Vliv na globální oteplování (GWP)","","","","675.0","675.0","675.0","675.0"]
["","Náplň","","","kg","1.50","1.50","1.50","1.50"]
["Hladina akustického výkonu","Jm.","","","dBA","39","39","39","39"]
["Provozní rozsah","Vytápění","Vody strana","Min.","°C","18","18","18","18"]
["","","","Max.","°C","65","65","65","65"]
["","Chlazení","Okolí","Min.","°CST","10","10","10","10"]
["","","Vody strana","Min.","°C","5","5","5","5"]
["","","","Max.","°C","22","22","22","22"]
["Napájení","Fáze","","","","1~","1~","1~","1~"]
["","Frekvence","","","Hz","50","50","50","50"]
["","Napětí","","","V","230","230","230","230"]
["Elektrický ohřívač","Napájení","","Název","","3V / 9W","3V / 9W","3V / 9W","3V / 9W"]
["","","","Fáze","","1~ / 3~","1~ / 3~","1~ / 3~","1~ / 3~"]
["","","","Frekvence","Hz","50","50","50","50"]
["Poznámky","","","","","(1) - Tepelná ztráta podle EN12897","(1) - Tepelná ztráta podle EN12897","(1) - Tepelná ztráta podle EN12897","(1) - Tepelná ztráta podle EN12897"]
["","","","","","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C","(2) - TKW = 10 °C/TWW = 40 °C/TSP = 50 °C"]
["","","","","","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60°C","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60°C","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60°C","(3) - TKW = 10 °C/TWW = 40 °C/TSP = 60°C"]
["","","","","","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65°C","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65°C","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65°C","(4) - TKW = 10 °C/TWW = 40 °C/TSP = 65°C"]
["","","","","","","(5) - Nahřátí zásobníku pouze tepelným čerpadlem, žádné elektrické ohřívání","","(5) - Nahřátí zásobníku pouze tepelným čerpadlem, žádné elektrické ohřívání"]