{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":17,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVH-E6V / ERGA04-08EVA"]
[]
[]
[]
[]
["","","","","","EHVH04S18EA6V / ERGA04EAV3A","EHVH04S23EA6V / ERGA04EAV3A","EHVH04S18EJ6V / ERGA04EAV3A","EHVH04S23EJ6V / ERGA04EAV3A","EHVH08S18EA6V / ERGA06EAV3A","EHVH08S23EA6V / ERGA06EAV3A","EHVH08S18EJ6V / ERGA06EAV3A","EHVH08S23EJ6V / ERGA06EAV3A","EHVH08S18EA6V / ERGA08EAV3A","EHVH08S18EJ6V / ERGA08EAV3A","EHVH08S23EA6V / ERGA08EAV3A","EHVH08S23EJ6V / ERGA08EAV3A"]
["Topný výkon","Jm.","","","kW","4.3 (1), 4.6 (2)","4.3 (1), 4.6 (2)","4.3 (1), 4.6 (2)","4.3 (1), 4.6 (2)","6.0 (1), 5.9 (2)","6.0 (1), 5.9 (2)","6.0 (1), 5.9 (2)","6.0 (1), 5.9 (2)","7.5 (1), 7.8 (2)","7.5 (1), 7.8 (2)","7.5 (1), 7.8 (2)","7.5 (1), 7.8 (2)"]
["Vstup napájení","Vytápění","","Jm.","kW","0.85 (1), 1.26 (2)","0.85 (1), 1.26 (2)","0.85 (1), 1.26 (2)","0.85 (1), 1.26 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)"]
["Příkon","Příkon-=-Teplá užitková voda od 10&nbsp;°C do 50&nbsp;°C","","Příkon-=-Teplá užitková voda od 10&nbsp;°C do 50&nbsp;°C-=-Jmen.-=-kWh","kWh","2.48","3.01","2.48","3.01","2.48","3.01","2.48","3.01","2.48","2.48","3.01","3.01"]
["Provoz vytápění od 10&nbsp;°C do 50&nbsp;°C.-=-hod.","hod.","","","","1h28min","1h40min","1h28min","1h40min","1h28min","1h40min","1h28min","1h40min","1h28min","1h28min","1h40min","1h40min"]
["COP","","","","","5.1 (1), 3.65 (2)","5.1 (1), 3.65 (2)","5.1 (1), 3.65 (2)","5.1 (1), 3.65 (2)","4.85 (1), 3.5 (2)","4.85 (1), 3.5 (2)","4.85 (1), 3.5 (2)","4.85 (1), 3.5 (2)","4.6 (1), 3.5 (2)","4.6 (1), 3.5 (2)","4.6 (1), 3.5 (2)","4.6 (1), 3.5 (2)"]
["Ohřev užitkové vody","Obecně","","Deklarovaný profil zátěže","","L","XL","L","XL","L","XL","L","XL","L","L","XL","XL"]
["","Průměrné podnebí","","Třída energetické účinnosti ohřevu vody","","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+"]
["Prostorové vytápění","Prostorové vytápění-=-Výstup vody 55&nbsp;°C v&nbsp;průměrném podnebí","Prostorové vytápění-=-Výstup vody 55&nbsp;°C v&nbsp;průměrném podnebí-=-Obecné","Prostorové vytápění-=-Výstup vody 55&nbsp;°C v&nbsp;průměrném podnebí-=-Obecné-=-SCOP","","3.26","3.26","3.26","3.26","3.25","3.25","3.25","3.25","3.27","3.27","3.27","3.27"]
["","","Prostorové vytápění-=-Výstup vody 55&nbsp;°C v&nbsp;průměrném podnebí-=-Obecně","Prostorové vytápění-=-Výstup vody 55&nbsp;°C v&nbsp;průměrném podnebí-=-Obecně-=-Třída celoroční účinnosti prostorového vytápění","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Prostorové vytápění-=-Výstup vody 35°C v&nbsp;průměrném podnebí","Prostorové vytápění-=-Výstup vody 35°C v&nbsp;průměrném podnebí-=-Obecné","Prostorové vytápění-=-Výstup vody 35°C v&nbsp;průměrném podnebí-=-Obecné-=-SCOP","","4.48","4.48","4.48","4.48","4.47","4.47","4.47","4.47","4.56","4.56","4.56","4.56"]
["","","","Prostorové vytápění-=-Výstup vody 35°C v&nbsp;průměrném podnebí-=-Obecné-=-Třída celoroční účinnosti prostorového vytápění","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Poznámky","","","","","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - Podmínky 2: chlazení Ta 35°C - LWE 7℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Podmínky 2: chlazení Ta 35°C - LWE 7℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Podmínky 2: chlazení Ta 35°C - LWE 7℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Podmínky 2: chlazení Ta 35°C - LWE 7℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Podmínky 2: chlazení Ta 35°C - LWE 7℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Podmínky 2: chlazení Ta 35°C - LWE 7℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Podmínky 2: chlazení Ta 35°C - LWE 7℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Podmínky 2: chlazení Ta 35°C - LWE 7℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Podmínky 2: chlazení Ta 35°C - LWE 7℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Podmínky 2: chlazení Ta 35°C - LWE 7℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Podmínky 2: chlazení Ta 35°C - LWE 7℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - Podmínky 2: chlazení Ta 35°C - LWE 7℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)"]