{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVZ-CB3V / ERHQ-BW17"]
[]
[]
[]
[]
["","","","","EHVZ16S18CB3V / ERHQ014BAW17"]
["Ohřev užitkové vody","Obecně","Deklarovaný profil zátěže","","L"]
["","Průměrné podnebí","Třída energetické účinnosti ohřevu vody","","A"]
["COP","","","","4.24 (1), 3.22 (2)"]
["Topný výkon","Jm.","","kW","14.5 (1), 13.6 (2)"]
["Příkon","Vytápění","Jm.","kW","3.42 (1), 4.21 (2)"]
["Poznámky","","","","(1) - Podmínky 1: chlazení Ta 35°C - LWE 18℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","(2) - Podmínky 2: chlazení Ta 35°C - LWE 7℃ (DT = 5°C); vytápění Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)"]
["","","","","(3) - Podmínky 3: vytápění Ta DB -7°C (RH85%) - LWC 35°C"]
["","","","","(4) - Podmínky 4: vytápění Ta DB -7°C (RH85%) - LWC 45℃"]
["","","","","(5) - Kapacita musí být rozložena mezi vedlejší a hlavní zónu Další informace o dostupném výkonu (kPa) jsou uvedeny v datech ESP."]
["","","","","(6) - DB/WB 7°C/6°C-LWC 35°C(DT=5°C)"]
["","","","","(7) - DB/WB 7°C/6°C - LWC 45℃ (Dt=5°C)"]
["","","","","(8) - 15 °C-25 °C: jen BUH, čerpadlo vytápění nefunguje = při zavádění"]