{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":6,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHH2E-AV3"]
[]
[]
[]
[]
["","","","","","EKHH2E260AAV3"]
["Sound power level","Ohřev užitkové vody","","Vnitřní jednotka","dBA","53"]
["","","","Venkovní jednotka","dBA","52"]
["Ohřev užitkové vody","Obecně","","Třída energetické účinnosti ohřevu vody","","A+"]
["","","","Nastavení teploty na termostatu","°C","55"]
["","","","Deklarovaný profil zátěže","","XL"]
["","Studené podnebí","","AEC (roční spotřeba elektřiny)","kWh","1,826"]
["","Teplé podnebí","","AEC (roční spotřeba elektřiny)","kWh","1,296"]
["","Průměrné podnebí","","AEC (roční spotřeba elektřiny)","kWh","1,323"]
["Ekvivalent vteplé vodě","Max.","","","l","342"]
["Čerpadlo vytápění","Automatic defrost start","","","°C","-2"]
["","Provozní rozsah","Okolí","Min.","°CST","-7"]
["","","","Max.","°CST","38"]
["","Casing","","Material","","Kryt: Povrchová vrstva z EPP"]
["","","","Barva","","White body / black top"]
["","Tlak v systému","","Max.","bar","7"]
["","Metoda odmrazování","","","","Aktivní s horkoplynovým ventilem"]
["COP","","","","","3.10 (1), 3.60 (2)"]
["Chladivo","Vliv na globální oteplování (GWP)","","","","1,430.0"]
["","Náplň","","","kg","0.900"]
["","Typ","","","","R-134a"]
["Kompresor","Typ","","","","Rotary non-inverter"]
["Rozměry","Jednotka","","Průměr","mm","650"]
["","","","Výška","mm","2,000"]
["Teplá užitková voda","Výkon","","Jmen.","kW","1.8"]
["Zásobník","Instalace","","Možnost připojení solárního tepelného systému","","Ne"]
["","Zabudované napájení topného prvku","","Jmen.","kW","1.5"]
["","Skříň","","Materiál","","Reliéfní ABS"]
["","","","Barva","","Bílá"]
["","Rozměry","Jednotka","Výška","mm","1,500"]
["","Provozní rozsah","Vody strana","Max.","°C","56"]
["","","","Min.","°C","10"]
["Hmotnost","Jednotka v obalu","","","kg","115"]
["","Jednotka","","Prázdná","kg","95"]
["","","","Plná","kg","349"]
["Místo instalace","","","","","Uvnitř"]
["IP class","","","","","IP-X4"]
["General","Product description","","Tepelné čerpadlo vzduch-voda","","Ano"]
["","Informace o dodavateli/výrobci","","Název a adresa","","ELIC - Via Pietro Zorutti 13/14, 33074 Fontanafredda ITALY"]
["Čas vytápění","Max.","","","hh:mm","10:14:00, 07:56:46"]
["Čerpadlo vytápění","Napájení","","Frekvence","Hz","50"]
["","","","Maximální proud při provozu","A","2"]
["","","","Fáze","","1P"]
["","","","Napětí","V","230"]
["Zásobník","Napájení","","Fáze","","1P"]
["","","","Frekvence","Hz","50"]
["","","","Napětí","V","230"]
["Poznámky","","","","","(1) - Podle EN16147-2011, vnitřní teplota 7°C, teplota místnosti 20°C, studená voda na vstupu 10°C"]
["","","","","","(2) - Podle EN16147-2011, vnitřní teplota 15°C, teplota místnosti 20°C, studená voda na vstupu 10°C"]
["","","","","","(3) - Vnitřní teplota: 29 ° CDB, 19 ° CWB; vnější teplota: 46 ° CDB, 24 ° CWB"]
["","","","","","(4) - Vnitřní teplota: 27 ° CDB, 19 ° CWB; vnější teplota: 35 ° CDB, 24 ° CWB"]