{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":7,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHHE-PCV3"]
[]
[]
[]
[]
["","","","","","EKHHE200PCV3","EKHHE260PCV3"]
["Sound power level","Ohřev užitkové vody","","Vnitřní jednotka","dBA","50","50"]
["","","","Venkovní jednotka","dBA","49","49"]
["Ohřev užitkové vody","Obecně","","Třída energetické účinnosti ohřevu vody","","A+","A+"]
["","","","Nastavení teploty na termostatu","°C","55","55"]
["","","","Funkce pro opravu ohřevu vody mimo špičku","","Ano","Ano"]
["","","","Deklarovaný profil zátěže","","L","XL"]
["","Studené podnebí","","AEC (roční spotřeba elektřiny)","kWh","979","1,672"]
["","","","Qelec (denní spotřeba elektřiny)","kWh","2.68","4.58"]
["","Teplé podnebí","","Qelec (denní spotřeba elektřiny)","kWh","1.91","3.10"]
["","","","AEC (roční spotřeba elektřiny)","kWh","698","1,132"]
["","Průměrné podnebí","","Qelec (denní spotřeba elektřiny)","kWh","2.08","3.30"]
["","","","AEC (roční spotřeba elektřiny)","kWh","758","1,203"]
["Čerpadlo vytápění","Provozní rozsah","Okolí","Min.","°CST","-7","-7"]
["","","","Max.","°CST","43","43"]
["","Casing","","Barva","","Bílá","Bílá"]
["","Tlak v systému","","Max.","bar","7","7"]
["","Metoda odmrazování","","","","Odmrazení horkým plynem","Odmrazení horkým plynem"]
["","Topný výkon","","","kW","0.43","0.43"]
["","Instalace","","Vzdálenost od stěny","mm","200","200"]
["","","","Krytí","","IP24","IP24"]
["","Hmotnost","","Jednotka","kg","96","106"]
["","","","Zabalená jednotka","kg","107","118"]
["","Místo instalace","","","","Pouze vnitřní","Pouze vnitřní"]
["","Hladina akustického tlaku","","Tichý noční režim","dBA","50.0","50.0"]
["","","","Jm.","dBA","50","50"]
["","Název","","","","EKHHE200PCV3","EKHHE260PCV3"]
["","Chladivo","","Vliv na globální oteplování (GWP)","","1,430","1,430"]
["","","","Náplň","kg","1","1"]
["","","","Typ","","R-134A","R-134A"]
["","Rozměry","Jednotka","Hloubka","mm","628","628"]
["","","","Šířka","mm","628","628"]
["","","","Výška","mm","1,607","1,892"]
["COP","","","","","4.23","4.23"]
["Chladivo","Vliv na globální oteplování (GWP)","","","","1,430","1,430"]
["","Náplň","","","kg","1","1"]
["","Typ","","","","R-134a","R-134a"]
["Kompresor","Typ","","","","Rotační","Rotační"]
["Rozměry","Jednotka","","Průměr","mm","628","628"]
["","","","Výška","mm","1,607","1,892"]
["","","Výška","Integrace na vnitřní jednotce","mm","1,607","1,892"]
["Teplá užitková voda","Výkon","","Jmen.","kW","1.82","1.82"]
["Nádrž","Instalace","","Možnost připojení solárního tepelného systému","","Ano","Ano"]
["","","","Krytí","","IP24","IP24"]
["","","","Otvor v nádrži pro recirkulaci","","Ne","Ne"]
["","Zabudované napájení topného prvku","","Jmen.","kW","1.5","1.5"]
["","Místo instalace","","","","Pouze vnitřní","Pouze vnitřní"]
["","Skříň","","Materiál","","Smaltovaná ocel","Smaltovaná ocel"]
["","","","Barva","","Bílá","Bílá"]
["","Název","","","","Smaltovaná ocelová nádrž 200 l","Smaltovaná ocelová nádrž 260 l"]
["Hmotnost","Jednotka v obalu","","","kg","107","118"]
["","Jednotka","","Prázdná","kg","96","106"]
["Místo instalace","","","","","Uvnitř","Uvnitř"]
["Obecně","LW (A) Hladina akustického výkonu (podle EN14825)","","Uvnitř","dB(A)","50","50"]
["","Popis výrobku","","Tepelné čerpadlo vzduch-voda","","Ano","Ano"]
["","","","Model identifier","","EKHHE200PCV3","EKHHE260PCV3"]
["","Informace ododavateli/výrobci","","Název nebo obchodní značka","","Daikin Europe N.V.","Daikin Europe N.V."]
["","Doplňkový ohřívač","","Typ příkonu","","Elektřina","Elektřina"]
["Čas vytápění","Max.","","","hh:mm","08:17:00","10:14:00"]
["Čerpadlo vytápění","Napájení","","Frekvence","Hz","50","50"]
["","","","Maximální proud při provozu","A","8.5","8.5"]
["","","","Fáze","","1P","1P"]
["","","","Napětí","V","230","230"]
["","","","Doporučená oblast použití","A","2.43","2.43"]
["Nádrž","Napájení","","Fáze","","1P","1P"]
["","","","Frekvence","Hz","50","50"]
["","","","Napětí","V","230","230"]