{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":7,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWET-BV3"]
[]
[]
[]
[]
["","","","","","EKHWET90BAV3","EKHWET120BAV3"]
["Upevnění","","","","","Stěna","Stěna"]
["Opláštění","Barva","","","","Bílá + černá","Bílá + černá"]
["","Materiál","","","","Plech, Akrylonitrile butadiene styren","Plech, Akrylonitrile butadiene styren"]
["Rozměry","Jednotka","Výška","Nádrž","mm","1032","1283"]
["","","","Šířka","mm","510","510"]
["","","","Hloubka","mm","570","570"]
["Hmotnost","Jednotka","","Prázdná","kg","43","47"]
["Nádrž","Objem vody","","","l","89","118"]
["","Materiál","","","","Smaltovaná ocel podle DIN 4753TL2","Smaltovaná ocel podle DIN 4753TL2"]
["Zásobník","Maximální teplota vody","","","°C","75.0","75.0"]
["","Třída energetické účinnosti","","","","B","C"]
["Tepelný výměník","Teplá užitková voda","","Množství","","1","1"]
["","","","Materiál trubek","","Hliník","Hliník"]
["","","","Provozní tlak","bar","42","42"]
["Pomocný ohřívač","Výkon","","","kW","1.2","1.2"]