{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":10,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWS-D3V3"]
[]
[]
[]
[]
["","","","","","EKHWS150D3V3","EKHWS180D3V3","EKHWS200D3V3","EKHWS250D3V3","EKHWS300D3V3"]
["Opláštění","Barva","","","","Neutrální bílá","Neutrální bílá","Neutrální bílá","Neutrální bílá","Neutrální bílá"]
["","Materiál","","","","Ocel natřená epoxidovou barvou, Nízkouhlíková ocel natřená epoxidovou barvou","Ocel natřená epoxidovou barvou, Nízkouhlíková ocel natřená epoxidovou barvou","Ocel natřená epoxidovou barvou, Nízkouhlíková ocel natřená epoxidovou barvou","Ocel natřená epoxidovou barvou, Nízkouhlíková ocel natřená epoxidovou barvou","Ocel natřená epoxidovou barvou, Nízkouhlíková ocel natřená epoxidovou barvou"]
["Rozměry","Jednotka","Výška","Nádrž","mm","1,000","1,164","1,264","1,535","1,745"]
["","","","Průměr","mm","595","595","595","595","595"]
["Hmotnost","Jednotka","","Prázdná","kg","45","50","53","58","63"]
["","","","Plná","kg","190","224","245","300","355"]
["Nádrž","Objem vody","","","l","145","174","192","242","292"]
["","Materiál","","","","Nerezová ocel (EN 1,4521)","Nerezová ocel (EN 1,4521)","Nerezová ocel (EN 1,4521)","Nerezová ocel (EN 1,4521)","Nerezová ocel (EN 1,4521)"]
["","Maximální teplota vody","","","°C","75","75","75","75","75"]
["","Třída energetické účinnosti","","","","B","B","B","B","B"]
["Výměník tepla","Teplá užitková voda","","Množství","","1","1","1","1","1"]
["","","","Materiál trubek","","Nerezová ocel (EN 1.4521)","Nerezová ocel (EN 1.4521)","Nerezová ocel (EN 1.4521)","Nerezová ocel (EN 1.4521)","Nerezová ocel (EN 1.4521)"]
["","","","Vnitřní objem výparníku","l","4.9","6.5","8.2","8.2","8.2"]
["","","","Provozní tlak","bar","10","10","10","10","10"]
["Pomocný ohřívač","Výkon","","","kW","3","3","3","3","3"]
["Poznámky","","","","","(1) - Tepelná ztráta podle EN12897","(1) - Tepelná ztráta podle EN12897","(1) - Tepelná ztráta podle EN12897","(1) - Tepelná ztráta podle EN12897","(1) - Tepelná ztráta podle EN12897"]