{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":7,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ELSXB-E"]
[]
[]
[]
[]
["","","","","","ELSXB12P50EF","ELSXB12P30EF"]
["Opláštění","Barva","","","","Dopravní bílá (RAL9016) / Dopravní černá (RAL9017)","Dopravní bílá (RAL9016) / Dopravní černá (RAL9017)"]
["","Materiál","","","","Polypropylén odolný proti nárazu","Polypropylén odolný proti nárazu"]
["Rozměry","Jednotka","","Výška","mm","1,910","1,893"]
["","","","Šířka","mm","792","594"]
["","","","Hloubka","mm","817","680"]
["Hmotnost","Jednotka","","","kg","91.0","76.0"]
["PED","Kategorie","","","","Kategorie II","Kategorie II"]
["Chladivo","Typ","","","","R-32","R-32"]
["Hladina akustického výkonu","Jm.","","","dBA","44.7","44.7"]
["Hladina akustického tlaku","Jm.","","","dBA","36.8","36.8"]
["Provozní rozsah","Vytápění","Vody strana","Min.","°C","15","15"]
["","","","Max.","°C","65","65"]
["","Chlazení","Okolí","Min.","°CST","10","10"]
["","","Vody strana","Min.","°C","5","5"]
["","","","Max.","°C","22","22"]
["Napájení","Fáze","","","","1~","1~"]
["","Frekvence","","","Hz","50","50"]
["","Napětí","","","V","230","230"]
["Poznámky","","","","","(1) - Provozní oblast je rozšířena na nižší průtoky v závislosti na provozním režimu – viz křivka ESP.","(1) - Provozní oblast je rozšířena na nižší průtoky v závislosti na provozním režimu – viz křivka ESP."]
["","","","","","(2) - Tepelná ztráta podle EN12897","(2) - Tepelná ztráta podle EN12897"]
["","","","","","(3) - Podrobnosti viz výkres provozních rozsahů","(3) - Podrobnosti viz výkres provozních rozsahů"]