{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERGA-EVH7"]
[]
[]
[]
[]
["","","","","","ERGA08EAV3H7"]
["Rozměry","Jednotka","","Výška","mm","740"]
["","","","Šířka","mm","884"]
["","","","Hloubka","mm","388"]
["Hmotnost","Jednotka","","","kg","58.5"]
["Provozní rozsah","Chlazení","","Min.","°CST","10"]
["","","","Max.","°CST","43"]
["","Teplá užitková voda","","Min.","°CST","-25"]
["","","","Max.","°CST","35"]
["Hladina akustického výkonu","Vytápění","","Jm.","dBA","62 (1)"]
["","Chlazení","","Jm.","dBA","62 (1)"]
["Hladina akustického tlaku","Vytápění","","Jm.","dBA","49 (1)"]
["","Chlazení","","Jm.","dBA","50 (1)"]
["Chladivo","Typ","","","","R-32"]
["","Vliv na globální oteplování (GWP)","","","","675.0"]
["","Náplň","","","tCO2Eq","1.01"]
["","Náplň","","","kg","1.50"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","6"]
["","Plyn","","Vnější průměr","mm","15.9"]
["Spoje potrubí","Vypouštění","","OD","mm","18"]
["","Rozdíl hladin","IU - OU","Max.","m","30.0"]
["Připojovací rozměry","Tepelná izolace","","","","Potrubí kapaliny a plynu"]
["Napájení","Označení","","","","V3"]
["","Fáze","","","","1N~"]
["","Frekvence","","","Hz","50"]
["","Napětí","","","V","230"]
["Proud","Doporučené jištění","","","A","25"]
["Poznámky","","","","","(1) - Chlazení Ta 35 °C - LWE 18℃ (DT = 5 °C); Vytápění Ta DB/WB 7 °C/6 °C - LWC 35℃ (DT = 5 °C)"]