{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERLA-DW17"]
[]
[]
[]
[]
["","","","","","ERLA16D2W17","ERLA16DAW17"]
["Rozměry","Jednotka","","Výška","mm","870","870"]
["","","","Šířka","mm","1,100","1,100"]
["","","","Hloubka","mm","460","460"]
["Hmotnost","Jednotka","","","kg","101","101"]
["Ventilátor","Průtok vzduchu","Vytápění","Vysoké","m³/min","85.0","85.0"]
["","","Chlazení","Vysoké","m³/min","85","85"]
["Provozní rozsah","Chlazení","","Min.","°CST","10","10"]
["","","","Max.","°CST","43","43"]
["","Teplá užitková voda","","Min.","°CST","-25","-25"]
["","","","Max.","°CST","25 (1), 35 (1)","25 (1), 35 (1)"]
["Hladina akustického výkonu","Vytápění","","Jm.","dBA","62.0 (2)","62.0 (2)"]
["Hladina akustického tlaku","Vytápění","","Jm.","dBA","48.0 (2)","48.0 (2)"]
["Chladivo","Typ","","","","R-32","R-32"]
["","Vliv na globální oteplování (GWP)","","","","675.0","675.0"]
["","Náplň","","","tCO2Eq","2.57","2.57"]
["","Náplň","","","kg","3.8","3.8"]
["Připojovací rozměry","Kapalina","","Vnější průměr","mm","9.5","9.5"]
["","Plyn","","Vnější průměr","mm","15.9","15.9"]
["Spoje potrubí","Vypouštění","","OD","mm","26","26"]
["","Rozdíl hladin","IU - OU","Max.","m","30.0","30.0"]
["Připojovací rozměry","Tepelná izolace","","","","Potrubí kapaliny a plynu","Potrubí kapaliny a plynu"]
["Napájení","Označení","","","","W1","W1"]
["","Fáze","","","","3~","3~"]
["","Frekvence","","","Hz","50","50"]
["","Napětí","","","V","400","400"]
["Proud","Doporučené jištění","","","A","16","16"]
["Poznámky","","","","","(1) - Podrobnosti viz výkres provozních rozsahů","(1) - Podrobnosti viz výkres provozních rozsahů"]
["","","","","","(2) - Měřeno při tlakové ztrátě 10 kPa v systému vytápění při teplotě vody na výstupu 47-55 °C v pokoji s teplotou 20 °C. DB/WB 7 °C/6°.","(2) - Měřeno při tlakové ztrátě 10 kPa v systému vytápění při teplotě vody na výstupu 47-55 °C v pokoji s teplotou 20 °C. DB/WB 7 °C/6°."]