{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERRQ-AY1"]
[]
[]
[]
[]
["","","","","","ERRQ011AAY1","ERRQ014AAY1","ERRQ016AAY1"]
["Hladina akustického tlaku","Vytápění","","Jm.","dBA","52","53","55"]
["Standardní příslušenství","Příručka pro instalaci","","","","1","1","1"]
["Hladina akustického výkonu","Vytápění","","Jm.","dBA","68","69","71"]
["Chladivo","Charge","","","TCO2Eq","9.4","9.4","9.4"]
["","GWP","","","","2,087.5","2,087.5","2,087.5"]
["","Náplň","","","kg","4.5","4.5","4.5"]
["","Type","","","","R-410A","R-410A","R-410A"]
["Rozměry","Jednotka","","Šířka","mm","900","900","900"]
["","","","Hloubka","mm","320","320","320"]
["","","","Výška","mm","1,345","1,345","1,345"]
["Provozní rozsah","Vytápění","","Max.","° CWB","20","20","20"]
["","","","Min.","° CWB","-20","-20","-20"]
["","Teplá užitková voda","","Min.","°CST","-20","-20","-20"]
["","","","Max.","°CST","35","35","35"]
["Hmotnost","Jednotka","","","kg","120","120","120"]
["Spoje potrubí","Tepelná izolace","","","","Potrubí kapaliny a plynu","Potrubí kapaliny a plynu","Potrubí kapaliny a plynu"]
["","Liquid","","OD","mm","9.52","9.52","9.52"]
["","Plyn","","OD","mm","15.9","15.9","15.9"]
["","Vypouštění","","OD","mm","26x3","26x3","26x3"]
["","Rozdíl hladin","IU - OU","Max.","m","30","30","30"]
["Power supply","Fáze","","","","3~","3~","3~"]
["","Frekvence","","","Hz","50","50","50"]
["","Name","","","","Y1","Y1","Y1"]
["","Napětí","","","V","380-415","380-415","380-415"]
["Proud","Doporučené jištění","","","A","16","16","16"]
["Poznámky","","","","","(1) - Viz samostatný výkres s provozním rozsahem","(1) - Viz samostatný výkres s provozním rozsahem","(1) - Viz samostatný výkres s provozním rozsahem"]
["","","","","","(2) - Obsahuje fluorované skleníkové plyny","(2) - Obsahuje fluorované skleníkové plyny","(2) - Obsahuje fluorované skleníkové plyny"]